AdapterId 061bfh

AdapterName "Intel SatisFAXtion Adapter"

NumBytes 4

NamedItem

Prompt "FAX I/O Address Range"

choice "0300h-030Fh,1300h-130Fh" pos[2]=10000XXXb io 0300h-030Fh 1300h-130Fh
choice "0310h-031Fh,1310h-131Fh" pos[2]=10001XXXb io 0310h-031Fh 1310h-131Fh
choice "0340h-034Fh,1340h-134Fh" pos[2]=10010XXXb io 0340h-034Fh 1340h-134Fh
choice "0350h-035Fh,1350h-135Fh" pos[2]=10011XXXb io 0350h-035Fh 1350h-135Fh
choice "0360h-036Fh,1360h-136Fh" pos[2]=10111XXXb io 0360h-036Fh 1360h-136Fh
choice "03A0h-03AFh,13A0h-13AFh" pos[2]=10100XXXb io 03A0h-03AFh 13A0h-13AFh
choice "03B0h-03BFh,13B0h-13BFh" pos[2]=10101XXXb io 03B0h-03BFh 13B0h-13BFh
choice "03E0h-03EFh,13E0h-13EFh" pos[2]=10110XXXb io 03E0h-03EFh 13E0h-13EFh
choice "0200h-020Fh,1200h-120Fh" pos[2]=11000XXXb io 0200h-020Fh 1200h-120Fh
choice "0210h-021Fh,1210h-121Fh" pos[2]=11001XXXb io 0210h-021Fh 1210h-121Fh
choice "0240h-024Fh,1240h-124Fh" pos[2]=11010XXXb io 0240h-024Fh 1240h-124Fh
choice "0250h-025Fh,1250h-125Fh" pos[2]=11011XXXb io 0250h-025Fh 1250h-125Fh
choice "02A0h-02AFh,12A0h-12AFh" pos[2]=11100XXXb io 02A0h-02AFh 12A0h-12AFh
choice "02B0h-02BFh,12B0h-12BFh" pos[2]=11101XXXb io 02B0h-02BFh 12B0h-12BFh
choice "02E0h-02EFh,12E0h-12EFh" pos[2]=11110XXXb io 02E0h-02EFh 12E0h-12EFh

Help
"
The software uses an I/O address to communicate with the Intel SatisFAXtion
adapter.  Always choose the default address (0300H-030FH,1300H-130FH) unless
that setting conflicts with another board's I/O address.  (Boards can't share
I/O addresses.)  An asterisk (*) appears if you choose an address already
used by another board.  If this happens, choose another address."


NamedItem

Prompt "Fax Interrupt Level"

choice "IRQ2"    pos[2]=XXXXX000b int 2
choice "IRQ3"    pos[2]=XXXXX001b int 3
choice "IRQ4"    pos[2]=XXXXX010b int 4
choice "IRQ5"    pos[2]=XXXXX011b int 5
choice "IRQ7"    pos[2]=XXXXX100b int 7

Help
"
The Intel SatisFAXtion adapter uses an interrupt to communicate with the
software.  This adapter's interrupt level can be shared with another device."

NamedItem

Prompt "Scanner I/O Address Range"

choice "0280h-0283h"    pos[3]=00100XXXb   io 0280h-0283h
choice "02A0h-02A3h"    pos[3]=00101XXXb   io 02A0h-02A3h
choice "02C0h-02C3h"    pos[3]=00110XXXb   io 02C0h-02C3h
choice "02E0h-02E3h"    pos[3]=00111XXXb   io 02E0h-02E3h
choice "0300h-0303h"    pos[3]=01000XXXb   io 0300h-0303h
choice "0320h-0323h"    pos[3]=01001XXXb   io 0320h-0323h
choice "0340h-0343h"    pos[3]=01010XXXb   io 0340h-0343h
choice "0360h-0363h"    pos[3]=01011XXXb   io 0360h-0363h
choice "0380h-0383h"    pos[3]=01100XXXb   io 0380h-0383h
choice "03A0h-03A3h"    pos[3]=01101XXXb   io 03A0h-03A3h
choice "03E0h-03E3h"    pos[3]=01111XXXb   io 03E0h-03E3h
choice "0200h-0203h"    pos[3]=00000XXXb   io 0200h-0203h
choice "0220h-0223h"    pos[3]=00001XXXb   io 0220h-0223h
choice "0240h-0243h"    pos[3]=00010XXXb   io 0240h-0243h
choice "0260h-0263h"    pos[3]=00011XXXb   io 0260h-0263h

Help
"
The software uses an I/O address to communicate with the Intel Hand Scanner.
Choose the default address (0280H-0283H) unless that setting conflicts with another
board's I/O address.  (Boards can't share I/O addresses.)  An asterisk (*)
appears if you choose an address already used by another board.  If this
happens, choose another address."

NamedItem

Prompt "Scanner Interrupt Level"

choice "Disabled"    pos[3]=0XXXX111b
choice "IRQ2"    pos[3]=0XXXX000b   int 2
choice "IRQ3"    pos[3]=0XXXX001b   int 3
choice "IRQ4"    pos[3]=0XXXX010b   int 4
choice "IRQ5"    pos[3]=0XXXX011b   int 5
choice "IRQ7"    pos[3]=0XXXX100b   int 7

Help
"
The Intel SatisFAXtion adapter uses an interrupt to communicate with the
software.  If you have the scanner option, choose the same interrupt as
in the Fax Interrupt Level field.  If you do not have the scanner option,
choose 'Disabled.'"
NamedItem

Prompt "Serial Port"

choice "SERIAL_1 " pos[1]=XXXX0000b io 03F8h-03FFh int 4
choice "SERIAL_2 " pos[1]=XXXX0001b io 02F8h-02FFh int 3
choice "SERIAL_3 " pos[1]=XXXX0010b io 3220h-3227h int 3
choice "SERIAL_4 " pos[1]=XXXX0011b io 3228h-322Fh int 3
choice "SERIAL_5 " pos[1]=XXXX0100b io 4220h-4227h int 3
choice "SERIAL_6 " pos[1]=XXXX0101b io 4228h-422Fh int 3
choice "SERIAL_7 " pos[1]=XXXX0110b io 5220h-5227h int 3
choice "SERIAL_8 " pos[1]=XXXX0111b io 5228h-522Fh int 3
choice "Disabled"  pos[1]=XXXX1XXXb

Help
"
The software uses a serial port to communicate with the modem.
If this is the only serial port in your computer, choose SERIAL_2
for the modem option.  Otherwise, choose SERIAL_3 through SERIAL_8.
(SERIAL_1 is usually used by the computer's built-in serial port.)
If you use a DOS-based communications program, you may not be able
to use SERIAL_3 through SERIAL_8.  SERIAL_1 and SERIAL_2 correspond to the
DOS ports COM1 and COM2 -- SERIAL_3 through SERIAL_8 have no
corresponding DOS ports.  Some DOS communications programs support
SERIAL_3 through SERIAL_8.  Don't choose SERIAL_3 through SERIAL_8
unless your communications program supports them.  An asterisk (*) appears
if you choose a serial port already being used.  If this happens, choose
another serial port."

NamedItem

Prompt "DMA Arbitration Level"

choice "Level 3" pos[1]=0XXXXXXXb pos[0]=11111111b arb 3
choice "Level 1" pos[1]=1XXXXXXXb pos[0]=11111111b arb 1

Help
"
The software uses a DMA channel to communicate with the Intel
SatisFAXtion adapter.  Always choose the default setting (DMA Channel 3)
unless that setting is being used by another board.  (Boards can't share
DMA channels.)  An asterisk (*) appears if you choose a DMA channel
already used by another board.  If this happens, choose another DMA
channel.  If neither of the DMA channels are available, change another
board's DMA channel so that Channel 3 or Channel 1 is available for the
Intel SatisFAXtion adapter."
