
AdapterID 0568bh

AdapterName  "MaynStream QIC-02 Tape Adapter"

NumBytes 2

nameditem
     Prompt  "Adapter Address"
	Choice "FF70H to FF77H" pos[0]=XXXXX10Xb io 0ff70h-0ff77h
	Choice "FF60H to FF67H" pos[0]=XXXXX00Xb io 0ff60h-0ff67h
	Help
	"The MaynStream QIC-02 Tape Adapter can reside at two different
	I/O addresses.	Select an address that does not conflict with
	other adapters.  An address conflict is indicated by an
	asterisk."


nameditem
     Prompt  "DMA Arbitration Levels"
	Choice	"Level 6"  pos[0]=110XXXXXb  arb 6
	Choice	"Level 5"  pos[0]=101XXXXXb  arb 5
	Choice	"Level 1"  pos[0]=001XXXXXb  arb 1
	Choice	"Level 3"  pos[0]=011XXXXXb  arb 3
	Choice	"Level 4"  pos[0]=100XXXXXb  arb 4
	Choice	"Level 7"  pos[0]=111XXXXXb  arb 7
	Choice	"Non-DMA mode" pos[0]=000XXXXXb
	Help
	"The MaynStream QIC-02 Tape Adapter can support several different
	DMA arbitration levels.  Select an arbitration level for the MaynStream
	QIC-02 Tape Adapter that does not conflict with other adapters. An
	arbitration conflict is indicated by an asterisk.  The non-DMA mode
	does not use DMA or interrupts."

nameditem
     Prompt  "Interrupt Level"
	Choice	"Level 2"  pos[0]=XXX00XXXb int 2
	Choice	"Level 3"  pos[0]=XXX01XXXb int 3
	Choice	"Level 5"  pos[0]=XXX10XXXb int 5
	Choice	"Level 7"  pos[0]=XXX11XXXb int 7
	Help
	"The MaynStream QIC-02 Tape Adapter can support several different
	interrupt levels.  Although it is unnecessary to use an unique
	interrupt, it is recommended that you do so."
