AdapterId 07F99h

AdapterName "DigiCHANNEL MC/4i or MC/8i   ( 32k Memory Window ) "

NumBytes 1

NamedItem

Prompt "Memory Start Address"

choice "0C0000" pos[0]=xxxxx00xb mem 00c0000h-00c7fffh

choice "0C8000" pos[0]=xxxxx01xb mem 00c8000h-00cffffh

choice "0D0000" pos[0]=xxxxx10xb mem 00d0000h-00d7fffh

choice "0D8000" pos[0]=xxxxx11xb mem 00d8000h-00dffffh 

Help

"Select one of four possible memory blocks where the MC/Xi will
 reside in the host memory map."

NamedItem

Prompt "I/O PORT Address"

choice "F1F0h" pos[0]=xxx00xxxb io 0f1f0h-0f1f1h

choice "F2F0h" pos[0]=xxx01xxxb io 0f2f0h-0f2f1h

choice "F4F0h" pos[0]=xxx10xxxb io 0f4f0h-0f4f1h

choice "F8F0h" pos[0]=xxx11xxxb io 0f8f0h-0f8f1h

Help

"Select one of four possible I/O locations where the MC/Xi will
 reside in the host I/O map."

NamedItem

Prompt "Interrupt Select"

choice "IRQ 11" pos[0]=111xxxxxb  int 11
choice "IRQ 10" pos[0]=110xxxxxb  int 10
choice "IRQ 5" pos[0]=010xxxxxb   int 5
choice "IRQ 4" pos[0]=001xxxxxb   int 4
choice "IRQ 9" pos[0]=101xxxxxb   int 9
choice "IRQ 7" pos[0]=100xxxxxb   int 7
choice "IRQ 6" pos[0]=011xxxxxb   int 6
choice "IRQ 3" pos[0]=000xxxxxb   int 3

Help

"Select one of eight possible Interrupt Request Lines on which the MC/Xi
 will interrupt the Host."