AdapterId 07081h

AdapterName "AST Advantage/2 -386 Adapter"

NumBytes 4

NamedItem
      Prompt "Memory size configuration "
      choice "MEMORY DISABLED"  POS[0]=X000XXXXb
      choice "1 MEGABYTES"      POS[0]=X001XXXXb
      choice "2 MEGABYTES"      POS[0]=X010XXXXb
      choice "4 MEGABYTES"      POS[0]=X011XXXXb
      choice "5 MEGABYTES"      POS[0]=X100XXXXb
      choice "8 MEGABYTES"      POS[0]=X101XXXXb


Help
" Memory Size Configuration indicates the amount of memory in
Bank0 and Bank1.  For one megabyte (MB), Bank0 is populated only.
Two MB's consists of Bank0 and Bank1 having one MB each.  Four MB's
consists of 4 MB's in Bank0 and none in Bank1.  Five MB's will have
one MB in Bank0 and four MB's in Bank1.  Eight MB's consists of four
MB's in Bank0 and four MB's in Bank1.   "

NamedItem
      Prompt "Wait State selection"
      choice "0 WAIT STATES"  pos[1]=1XXXXXXXb
      choice "1 WAIT STATE"   pos[1]=0XXXXXXXb

Help
" An additional wait state is inserted during any memory access when
  the choice '1 WAIT STATE' is made ."

NamedItem
     Prompt "Connector 1"
	choice "SERIAL_1"
		      pos[2]=1000XXXXb
		      pos[3]=xx1xxxxxb
		      io 03f8h-03ffh int 4
	choice "SERIAL_2"
		      pos[2]=1001XXXXb
		      pos[3]=xx1xxxxxb
		      io 02f8h-02ffh int 3
	choice "SERIAL_3"
		      pos[2]=1010XXXXb
		      pos[3]=xx1xxxxxb
		      io 3220h-3227h int 3
	choice "SERIAL_4"
		      pos[2]=1011XXXXb
		      pos[3]=xx1xxxxxb
		      io 3228h-322fh int 3
	choice "SERIAL_5"
		      pos[2]=1100XXXXb
		      pos[3]=xx1xxxxxb
		      io 4220h-4227h int 3
	choice "SERIAL_6"
		      pos[2]=1101XXXXb
		      pos[3]=xx1xxxxxb
		      io 4228h-422fh int 3
	choice "SERIAL_7"
		      pos[2]=1110XXXXb
		      pos[3]=xx1xxxxxb
		      io 5220h-5227h int 3
	choice "SERIAL_8"
		      pos[2]=1111XXXXb
		      pos[3]=xx1xxxxxb
		      io 5228h-522fh int 3
	choice "DISABLE"
		      pos[3]=xx0xxxxxb
   Help
      "Connector 1 of  Advantage/2 Serial  and  Parallel Port
      Option can have  any one of the  Serial 1  to  Serial 8
      assignments  and	can  also  be  disabled.  Use the F5=
      Previous and the F6=Next keys to change the Connector 1
      Serial port assignments  when  you  are  in the 'Change
      Configuration'  window.   Conflicting  assignments  are
      marked with an Asterisk and should be changed."

NamedItem
     Prompt "Connector 2"
	choice "SERIAL_1"
		      pos[2]=XXXX000Xb
		      pos[3]=xxx1xxxxb
		      io 03f8h-03ffh int 4
	choice "SERIAL_2"
		      pos[2]=XXXX001Xb
		      pos[3]=xxx1xxxxb
		      io 02f8h-02ffh int 3
	choice "SERIAL_3"
		      pos[2]=XXXX010Xb
		      pos[3]=xxx1xxxxb
		      io 3220h-3227h int 3
	choice "SERIAL_4"
		      pos[2]=XXXX011Xb
		      pos[3]=xxx1xxxxb
		      io 3228h-322fh int 3
	choice "SERIAL_5"
		      pos[2]=XXXX100Xb
		      pos[3]=xxx1xxxxb
		      io 4220h-4227h int 3
	choice "SERIAL_6"
		      pos[2]=XXXX101Xb
		      pos[3]=xxx1xxxxb
		      io 4228h-422fh int 3
	choice "SERIAL_7"
		      pos[2]=XXXX110Xb
		      pos[3]=xxx1xxxxb
		      io 5220h-5227h int 3
	choice "SERIAL_8"
		      pos[2]=XXXX111Xb
		      pos[3]=xxx1xxxxb
		      io 5228h-522fh int 3
	choice "DISABLE"
		      pos[3]=xxx0xxxxb
     Help
	"Connector 2 of the AST Advantage/2 Dual Serial Port
	Option can have any one of the Serial 1 to  Serial 8
	assignment and can  also be  disabled.	Use the  F5=
	Previous and F6=Next keys to change the  Connector 2
	Serial Port assignment	when you are in the  'Change
	Configuration' window.  Conflicting  assignments are
	marked with an asterisk and should be changed."


