;Hayes Smartmodem 2400P Option Diskette 96-00128 V1.0
;(c) 1988 Hayes Microcomputer Products, Inc.

AdapterId 06F01H

AdapterName "Hayes Smartmodem 2400P"

NumBytes 1

NamedItem

Prompt "Communication Port"

choice "SERIAL_1" pos[1]=XXXX1000b io 03f8h-03ffh int 4
choice "SERIAL_2" pos[1]=XXXX1001b io 02f8h-02ffh int 3
choice "SERIAL_3" pos[1]=XXXX1010b io 3220h-3227h int 3
choice "SERIAL_4" pos[1]=XXXX1011b io 3228h-322fh int 3
choice "SERIAL_5" pos[1]=XXXX1100b io 4220h-4227h int 3
choice "SERIAL_6" pos[1]=XXXX1101b io 4228h-422fh int 3
choice "SERIAL_7" pos[1]=XXXX1110b io 5220h-5227h int 3
choice "SERIAL_8" pos[1]=XXXX1111b io 5228h-522fh int 3

Help

"The Hayes Smartmodem 2400P can be assigned to Communication
Ports SERIAL_1 through SERIAL_8.  If you will be using Hayes
Smartcom II or Smartcom III, be sure to select SERIAL_1 (COM1) or
SERIAL_2 (COM2).  To change the assignment use the F5=Previous
and the F6=Next keys."
