
AdapterId 06508H

AdapterName  "PDIuC508 Microchannel ARCNET Interface Adapter"

NumBytes 3

NamedItem

      Prompt "Memory base address"
	choice "0D0000h"  pos[0]=100XXXX1b MEM 0D0000H - 0D3FFFH
	choice "0D4000h"  pos[0]=101XXXX1b MEM 0D4000H - 0D7FFFH
	choice "0D8000h"  pos[0]=110XXXX1b MEM 0D8000H - 0DBFFFH
	choice "0DC000h"  pos[0]=111XXXX1b MEM 0DC000H - 0DFFFFH
	choice "0C0000h"  pos[0]=000XXXX1b MEM 0C0000H - 0C3FFFH
	choice "0C4000h"  pos[0]=001XXXX1b MEM 0C4000H - 0C7FFFH
	choice "0C8000h"  pos[0]=010XXXX1b MEM 0C8000H - 0CBFFFH
	choice "0CC000h"  pos[0]=011XXXX1b MEM 0CC000H - 0CFFFFH

      Help
      "To configure this adapter you must choose the memory location
       the adapter will use for its packet buffer.  There are eight
       memory locations that can be selected.  The default memory
       base address for ARCNET is at 0D0000h.  Use the F5=Previous,
       F6=Next keys to change this assignment.	Conflicting assignments
       are marked with an asterisk and must be changed."


NamedItem

      Prompt "Interrupt Level"
	choice "9  "                pos[0]=XXX10011b INT 9
	choice "10 "                pos[0]=XXX10101b INT 10
	choice "11 "                pos[0]=XXX10111b INT 11
	choice "12 "                pos[0]=XXX11001b INT 12
	choice "14 "                pos[0]=XXX11101b INT 14
	choice "15 "                pos[0]=XXX11111b INT 15
	choice "interrupt not used" pos[0]=XXX00001b
	choice "3  "                pos[0]=XXX00111b INT 3
	choice "4  "                pos[0]=XXX01001b INT 4
	choice "5  "                pos[0]=XXX01011b INT 5
	choice "6  "                pos[0]=XXX01101b INT 6
	choice "7  "                pos[0]=XXX01111b INT 7

      Help
      "To configure this adapter you must choose the interrupt level
       the adapter will use.  The choice 'interrupt not used' should
       not be used under normal circumstances.	There are twelve
       interrupt levels that can be selected.  The default interrupt
       level for ARCNET is 9.  Use the F5=Previous, F6=Next keys to
       change this assignment.	Conflicting assignments are marked
       with an asterisk and must be changed."

NamedItem

      Prompt "I/O Base Address"
	choice "02E0h"  pos[1]=XX101110b IO 02E0H - 02EFH
	choice "02F0h"  pos[1]=XX101111b IO 02F0H - 02FFH
	choice "0300h"  pos[1]=XX110000b IO 0300H - 030FH
	choice "0310h"  pos[1]=XX110001b IO 0310H - 031FH
	choice "0320h"  pos[1]=XX110010b IO 0320H - 032FH
	choice "0330h"  pos[1]=XX110011b IO 0330H - 033FH
	choice "0340h"  pos[1]=XX110100b IO 0340H - 034FH
	choice "0350h"  pos[1]=XX110101b IO 0350H - 035FH
	choice "0360h"  pos[1]=XX110110b IO 0360H - 036FH
	choice "0370h"  pos[1]=XX110111b IO 0370H - 037FH
	choice "0380h"  pos[1]=XX111000b IO 0380H - 038FH
	choice "0390h"  pos[1]=XX111001b IO 0390H - 039FH
	choice "03A0h"  pos[1]=XX111010b IO 03A0H - 03AFH
	choice "03B0h"  pos[1]=XX111011b IO 03B0H - 03BFH
	choice "03C0h"  pos[1]=XX111100b IO 03C0H - 03CFH
	choice "03D0h"  pos[1]=XX111101b IO 03D0H - 03DFH
	choice "03E0h"  pos[1]=XX111110b IO 03E0H - 03EFH
	choice "03F0h"  pos[1]=XX111111b IO 03F0H - 03FFH
	choice "0200h"  pos[1]=XX100000b IO 0200H - 020FH
	choice "0210h"  pos[1]=XX100001b IO 0210H - 021FH
	choice "0220h"  pos[1]=XX100010b IO 0220H - 022FH
	choice "0230h"  pos[1]=XX100011b IO 0230H - 023FH
	choice "0240h"  pos[1]=XX100100b IO 0240H - 024FH
	choice "0250h"  pos[1]=XX100101b IO 0250H - 025FH
	choice "0260h"  pos[1]=XX100110b IO 0260H - 026FH
	choice "0270h"  pos[1]=XX100111b IO 0270H - 027FH
	choice "0280h"  pos[1]=XX101000b IO 0280H - 028FH
	choice "0290h"  pos[1]=XX101001b IO 0290H - 029FH
	choice "02A0h"  pos[1]=XX101010b IO 02A0H - 02AFH
	choice "02B0h"  pos[1]=XX101011b IO 02B0H - 02BFH
	choice "02C0h"  pos[1]=XX101100b IO 02C0H - 02CFH
	choice "02D0h"  pos[1]=XX101101b IO 02D0H - 02DFH

      Help
      "To configure this adapter you must choose the I/O address
       the adapter will use for its operation. There are thirty two
       I/O locations that can be selected.  The default I/O
       base address for ARCNET is at 02E0h.  Use the F5=Previous,
       F6=Next keys to change this assignment.	Conflicting assignments
       are marked with an asterisk and must be changed."


NamedItem

      Prompt "ARCNET Response Time"
	choice "74.7 uS  "   pos[1]=11XXXXXXb
	choice "283.4 uS "   pos[1]=10XXXXXXb
	choice "561.8 uS "   pos[1]=01XXXXXXb
	choice "1118.6 uS"   pos[1]=00XXXXXXb


      Help
"Use F5 and F6 to select the ARCNET response time.  Response time of
74.7 uS is used typically.  Longer response time is required only if the
longest distance between any 2 nodes is more than 4 miles when RG62
co-axial cable is used.  Adapters in the same network must have the same
response time."


NamedItem

      Prompt "ARCNET Node Address"

	choice "decimal 128, hex 80h"  pos[2]=10000000b
	choice "decimal 129, hex 81h"  pos[2]=10000001b
	choice "decimal 130, hex 82h"  pos[2]=10000010b
	choice "decimal 131, hex 83h"  pos[2]=10000011b
	choice "decimal 132, hex 84h"  pos[2]=10000100b
	choice "decimal 133, hex 85h"  pos[2]=10000101b
	choice "decimal 134, hex 86h"  pos[2]=10000110b
	choice "decimal 135, hex 87h"  pos[2]=10000111b
	choice "decimal 136, hex 88h"  pos[2]=10001000b
	choice "decimal 137, hex 89h"  pos[2]=10001001b
	choice "decimal 138, hex 8Ah"  pos[2]=10001010b
	choice "decimal 139, hex 8Bh"  pos[2]=10001011b
	choice "decimal 140, hex 8Ch"  pos[2]=10001100b
	choice "decimal 141, hex 8Dh"  pos[2]=10001101b
	choice "decimal 142, hex 8Eh"  pos[2]=10001110b
	choice "decimal 143, hex 8Fh"  pos[2]=10001111b

	choice "decimal 144, hex 90h"  pos[2]=10010000b
	choice "decimal 145, hex 91h"  pos[2]=10010001b
	choice "decimal 146, hex 92h"  pos[2]=10010010b
	choice "decimal 147, hex 93h"  pos[2]=10010011b
	choice "decimal 148, hex 94h"  pos[2]=10010100b
	choice "decimal 149, hex 95h"  pos[2]=10010101b
	choice "decimal 150, hex 96h"  pos[2]=10010110b
	choice "decimal 151, hex 97h"  pos[2]=10010111b
	choice "decimal 152, hex 98h"  pos[2]=10011000b
	choice "decimal 153, hex 99h"  pos[2]=10011001b
	choice "decimal 154, hex 9Ah"  pos[2]=10011010b
	choice "decimal 155, hex 9Bh"  pos[2]=10011011b
	choice "decimal 156, hex 9Ch"  pos[2]=10011100b
	choice "decimal 157, hex 9Dh"  pos[2]=10011101b
	choice "decimal 158, hex 9Eh"  pos[2]=10011110b
	choice "decimal 159, hex 9Fh"  pos[2]=10011111b

	choice "decimal 160, hex A0h"  pos[2]=10100000b
	choice "decimal 161, hex A1h"  pos[2]=10100001b
	choice "decimal 162, hex A2h"  pos[2]=10100010b
	choice "decimal 163, hex A3h"  pos[2]=10100011b
	choice "decimal 164, hex A4h"  pos[2]=10100100b
	choice "decimal 165, hex A5h"  pos[2]=10100101b
	choice "decimal 166, hex A6h"  pos[2]=10100110b
	choice "decimal 167, hex A7h"  pos[2]=10100111b
	choice "decimal 168, hex A8h"  pos[2]=10101000b
	choice "decimal 169, hex A9h"  pos[2]=10101001b
	choice "decimal 170, hex AAh"  pos[2]=10101010b
	choice "decimal 171, hex ABh"  pos[2]=10101011b
	choice "decimal 172, hex ACh"  pos[2]=10101100b
	choice "decimal 173, hex ADh"  pos[2]=10101101b
	choice "decimal 174, hex AEh"  pos[2]=10101110b
	choice "decimal 175, hex AFh"  pos[2]=10101111b

	choice "decimal 176, hex B0h"  pos[2]=10110000b
	choice "decimal 177, hex B1h"  pos[2]=10110001b
	choice "decimal 178, hex B2h"  pos[2]=10110010b
	choice "decimal 179, hex B3h"  pos[2]=10110011b
	choice "decimal 180, hex B4h"  pos[2]=10110100b
	choice "decimal 181, hex B5h"  pos[2]=10110101b
	choice "decimal 182, hex B6h"  pos[2]=10110110b
	choice "decimal 183, hex B7h"  pos[2]=10110111b
	choice "decimal 184, hex B8h"  pos[2]=10111000b
	choice "decimal 185, hex B9h"  pos[2]=10111001b
	choice "decimal 186, hex BAh"  pos[2]=10111010b
	choice "decimal 187, hex BBh"  pos[2]=10111011b
	choice "decimal 188, hex BCh"  pos[2]=10111100b
	choice "decimal 189, hex BDh"  pos[2]=10111101b
	choice "decimal 190, hex BEh"  pos[2]=10111110b
	choice "decimal 191, hex BFh"  pos[2]=10111111b

	choice "decimal 192, hex C0h"  pos[2]=11000000b
	choice "decimal 193, hex C1h"  pos[2]=11000001b
	choice "decimal 194, hex C2h"  pos[2]=11000010b
	choice "decimal 195, hex C3h"  pos[2]=11000011b
	choice "decimal 196, hex C4h"  pos[2]=11000100b
	choice "decimal 197, hex C5h"  pos[2]=11000101b
	choice "decimal 198, hex C6h"  pos[2]=11000110b
	choice "decimal 199, hex C7h"  pos[2]=11000111b
	choice "decimal 200, hex C8h"  pos[2]=11001000b
	choice "decimal 201, hex C9h"  pos[2]=11001001b
	choice "decimal 202, hex CAh"  pos[2]=11001010b
	choice "decimal 203, hex CBh"  pos[2]=11001011b
	choice "decimal 204, hex CCh"  pos[2]=11001100b
	choice "decimal 205, hex CDh"  pos[2]=11001101b
	choice "decimal 206, hex CEh"  pos[2]=11001110b
	choice "decimal 207, hex CFh"  pos[2]=11001111b

	choice "decimal 208, hex D0h"  pos[2]=11010000b
	choice "decimal 209, hex D1h"  pos[2]=11010001b
	choice "decimal 210, hex D2h"  pos[2]=11010010b
	choice "decimal 211, hex D3h"  pos[2]=11010011b
	choice "decimal 212, hex D4h"  pos[2]=11010100b
	choice "decimal 213, hex D5h"  pos[2]=11010101b
	choice "decimal 214, hex D6h"  pos[2]=11010110b
	choice "decimal 215, hex D7h"  pos[2]=11010111b
	choice "decimal 216, hex D8h"  pos[2]=11011000b
	choice "decimal 217, hex D9h"  pos[2]=11011001b
	choice "decimal 218, hex DAh"  pos[2]=11011010b
	choice "decimal 219, hex DBh"  pos[2]=11011011b
	choice "decimal 220, hex DCh"  pos[2]=11011100b
	choice "decimal 221, hex DDh"  pos[2]=11011101b
	choice "decimal 222, hex DEh"  pos[2]=11011110b
	choice "decimal 223, hex DFh"  pos[2]=11011111b

	choice "decimal 224, hex E0h"  pos[2]=11100000b
	choice "decimal 225, hex E1h"  pos[2]=11100001b
	choice "decimal 226, hex E2h"  pos[2]=11100010b
	choice "decimal 227, hex E3h"  pos[2]=11100011b
	choice "decimal 228, hex E4h"  pos[2]=11100100b
	choice "decimal 229, hex E5h"  pos[2]=11100101b
	choice "decimal 230, hex E6h"  pos[2]=11100110b
	choice "decimal 231, hex E7h"  pos[2]=11100111b
	choice "decimal 232, hex E8h"  pos[2]=11101000b
	choice "decimal 233, hex E9h"  pos[2]=11101001b
	choice "decimal 234, hex EAh"  pos[2]=11101010b
	choice "decimal 235, hex EBh"  pos[2]=11101011b
	choice "decimal 236, hex ECh"  pos[2]=11101100b
	choice "decimal 237, hex EDh"  pos[2]=11101101b
	choice "decimal 238, hex EEh"  pos[2]=11101110b
	choice "decimal 239, hex EFh"  pos[2]=11101111b

	choice "decimal 240, hex F0h"  pos[2]=11110000b
	choice "decimal 241, hex F1h"  pos[2]=11110001b
	choice "decimal 242, hex F2h"  pos[2]=11110010b
	choice "decimal 243, hex F3h"  pos[2]=11110011b
	choice "decimal 244, hex F4h"  pos[2]=11110100b
	choice "decimal 245, hex F5h"  pos[2]=11110101b
	choice "decimal 246, hex F6h"  pos[2]=11110110b
	choice "decimal 247, hex F7h"  pos[2]=11110111b
	choice "decimal 248, hex F8h"  pos[2]=11111000b
	choice "decimal 249, hex F9h"  pos[2]=11111001b
	choice "decimal 250, hex FAh"  pos[2]=11111010b
	choice "decimal 251, hex FBh"  pos[2]=11111011b
	choice "decimal 252, hex FCh"  pos[2]=11111100b
	choice "decimal 253, hex FDh"  pos[2]=11111101b
	choice "decimal 254, hex FEh"  pos[2]=11111110b
	choice "decimal 255, hex FFh"  pos[2]=11111111b

	choice "decimal 001, hex 01h"  pos[2]=00000001b
	choice "decimal 002, hex 02h"  pos[2]=00000010b
	choice "decimal 003, hex 03h"  pos[2]=00000011b
	choice "decimal 004, hex 04h"  pos[2]=00000100b
	choice "decimal 005, hex 05h"  pos[2]=00000101b
	choice "decimal 006, hex 06h"  pos[2]=00000110b
	choice "decimal 007, hex 07h"  pos[2]=00000111b
	choice "decimal 008, hex 08h"  pos[2]=00001000b
	choice "decimal 009, hex 09h"  pos[2]=00001001b
	choice "decimal 010, hex 0Ah"  pos[2]=00001010b
	choice "decimal 011, hex 0Bh"  pos[2]=00001011b
	choice "decimal 012, hex 0Ch"  pos[2]=00001100b
	choice "decimal 013, hex 0Dh"  pos[2]=00001101b
	choice "decimal 014, hex 0Eh"  pos[2]=00001110b
	choice "decimal 015, hex 0Fh"  pos[2]=00001111b

	choice "decimal 016, hex 10h"  pos[2]=00010000b
	choice "decimal 017, hex 11h"  pos[2]=00010001b
	choice "decimal 018, hex 12h"  pos[2]=00010010b
	choice "decimal 019, hex 13h"  pos[2]=00010011b
	choice "decimal 020, hex 14h"  pos[2]=00010100b
	choice "decimal 021, hex 15h"  pos[2]=00010101b
	choice "decimal 022, hex 16h"  pos[2]=00010110b
	choice "decimal 023, hex 17h"  pos[2]=00010111b
	choice "decimal 024, hex 18h"  pos[2]=00011000b
	choice "decimal 025, hex 19h"  pos[2]=00011001b
	choice "decimal 026, hex 1Ah"  pos[2]=00011010b
	choice "decimal 027, hex 1Bh"  pos[2]=00011011b
	choice "decimal 028, hex 1Ch"  pos[2]=00011100b
	choice "decimal 029, hex 1Dh"  pos[2]=00011101b
	choice "decimal 030, hex 1Eh"  pos[2]=00011110b
	choice "decimal 031, hex 1Fh"  pos[2]=00011111b

	choice "decimal 032, hex 20h"  pos[2]=00100000b
	choice "decimal 033, hex 21h"  pos[2]=00100001b
	choice "decimal 034, hex 22h"  pos[2]=00100010b
	choice "decimal 035, hex 23h"  pos[2]=00100011b
	choice "decimal 036, hex 24h"  pos[2]=00100100b
	choice "decimal 037, hex 25h"  pos[2]=00100101b
	choice "decimal 038, hex 26h"  pos[2]=00100110b
	choice "decimal 039, hex 27h"  pos[2]=00100111b
	choice "decimal 040, hex 28h"  pos[2]=00101000b
	choice "decimal 041, hex 29h"  pos[2]=00101001b
	choice "decimal 042, hex 2Ah"  pos[2]=00101010b
	choice "decimal 043, hex 2Bh"  pos[2]=00101011b
	choice "decimal 044, hex 2Ch"  pos[2]=00101100b
	choice "decimal 045, hex 2Dh"  pos[2]=00101101b
	choice "decimal 046, hex 2Eh"  pos[2]=00101110b
	choice "decimal 047, hex 2Fh"  pos[2]=00101111b

	choice "decimal 048, hex 30h"  pos[2]=00110000b
	choice "decimal 049, hex 31h"  pos[2]=00110001b
	choice "decimal 050, hex 32h"  pos[2]=00110010b
	choice "decimal 051, hex 33h"  pos[2]=00110011b
	choice "decimal 052, hex 34h"  pos[2]=00110100b
	choice "decimal 053, hex 35h"  pos[2]=00110101b
	choice "decimal 054, hex 36h"  pos[2]=00110110b
	choice "decimal 055, hex 37h"  pos[2]=00110111b
	choice "decimal 056, hex 38h"  pos[2]=00111000b
	choice "decimal 057, hex 39h"  pos[2]=00111001b
	choice "decimal 058, hex 3Ah"  pos[2]=00111010b
	choice "decimal 059, hex 3Bh"  pos[2]=00111011b
	choice "decimal 060, hex 3Ch"  pos[2]=00111100b
	choice "decimal 061, hex 3Dh"  pos[2]=00111101b
	choice "decimal 062, hex 3Eh"  pos[2]=00111110b
	choice "decimal 063, hex 3Fh"  pos[2]=00111111b

	choice "decimal 064, hex 40h"  pos[2]=01000000b
	choice "decimal 065, hex 41h"  pos[2]=01000001b
	choice "decimal 066, hex 42h"  pos[2]=01000010b
	choice "decimal 067, hex 43h"  pos[2]=01000011b
	choice "decimal 068, hex 44h"  pos[2]=01000100b
	choice "decimal 069, hex 45h"  pos[2]=01000101b
	choice "decimal 070, hex 46h"  pos[2]=01000110b
	choice "decimal 071, hex 47h"  pos[2]=01000111b
	choice "decimal 072, hex 48h"  pos[2]=01001000b
	choice "decimal 073, hex 49h"  pos[2]=01001001b
	choice "decimal 074, hex 4Ah"  pos[2]=01001010b
	choice "decimal 075, hex 4Bh"  pos[2]=01001011b
	choice "decimal 076, hex 4Ch"  pos[2]=01001100b
	choice "decimal 077, hex 4Dh"  pos[2]=01001101b
	choice "decimal 078, hex 4Eh"  pos[2]=01001110b
	choice "decimal 079, hex 4Fh"  pos[2]=01001111b

	choice "decimal 080, hex 50h"  pos[2]=01010000b
	choice "decimal 081, hex 51h"  pos[2]=01010001b
	choice "decimal 082, hex 52h"  pos[2]=01010010b
	choice "decimal 083, hex 53h"  pos[2]=01010011b
	choice "decimal 084, hex 54h"  pos[2]=01010100b
	choice "decimal 085, hex 55h"  pos[2]=01010101b
	choice "decimal 086, hex 56h"  pos[2]=01010110b
	choice "decimal 087, hex 57h"  pos[2]=01010111b
	choice "decimal 088, hex 58h"  pos[2]=01011000b
	choice "decimal 089, hex 59h"  pos[2]=01011001b
	choice "decimal 090, hex 5Ah"  pos[2]=01011010b
	choice "decimal 091, hex 5Bh"  pos[2]=01011011b
	choice "decimal 092, hex 5Ch"  pos[2]=01011100b
	choice "decimal 093, hex 5Dh"  pos[2]=01011101b
	choice "decimal 094, hex 5Eh"  pos[2]=01011110b
	choice "decimal 095, hex 5Fh"  pos[2]=01011111b

	choice "decimal 096, hex 60h"  pos[2]=01100000b
	choice "decimal 097, hex 61h"  pos[2]=01100001b
	choice "decimal 098, hex 62h"  pos[2]=01100010b
	choice "decimal 099, hex 63h"  pos[2]=01100011b
	choice "decimal 100, hex 64h"  pos[2]=01100100b
	choice "decimal 101, hex 65h"  pos[2]=01100101b
	choice "decimal 102, hex 66h"  pos[2]=01100110b
	choice "decimal 103, hex 67h"  pos[2]=01100111b
	choice "decimal 104, hex 68h"  pos[2]=01101000b
	choice "decimal 105, hex 69h"  pos[2]=01101001b
	choice "decimal 106, hex 6Ah"  pos[2]=01101010b
	choice "decimal 107, hex 6Bh"  pos[2]=01101011b
	choice "decimal 108, hex 6Ch"  pos[2]=01101100b
	choice "decimal 109, hex 6Dh"  pos[2]=01101101b
	choice "decimal 110, hex 6Eh"  pos[2]=01101110b
	choice "decimal 111, hex 6Fh"  pos[2]=01101111b

	choice "decimal 112, hex 70h"  pos[2]=01110000b
	choice "decimal 113, hex 71h"  pos[2]=01110001b
	choice "decimal 114, hex 72h"  pos[2]=01110010b
	choice "decimal 115, hex 73h"  pos[2]=01110011b
	choice "decimal 116, hex 74h"  pos[2]=01110100b
	choice "decimal 117, hex 75h"  pos[2]=01110101b
	choice "decimal 118, hex 76h"  pos[2]=01110110b
	choice "decimal 119, hex 77h"  pos[2]=01110111b
	choice "decimal 120, hex 78h"  pos[2]=01111000b
	choice "decimal 121, hex 79h"  pos[2]=01111001b
	choice "decimal 122, hex 7Ah"  pos[2]=01111010b
	choice "decimal 123, hex 7Bh"  pos[2]=01111011b
	choice "decimal 124, hex 7Ch"  pos[2]=01111100b
	choice "decimal 125, hex 7Dh"  pos[2]=01111101b
	choice "decimal 126, hex 7Eh"  pos[2]=01111110b
	choice "decimal 127, hex 7Fh"  pos[2]=01111111b


      Help
"Use F5 and F6 to select the ARCNET node address.  Each station
attached to the ARCNET local area network must have a unique
node address."

