; 
;	$Revision:   1.3  $
;	$Date:   09 Dec 1991 15:09:04  $
; 
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  			   *
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterID 0ddffh

ADAPTERNAME "ESDI Fixed Disk Controller"

NUMBYTES 2

FIXEDRESOURCES   pos[0]=XXXXXX0Xb   pos[1]=00XXXXXXb   io 3510h-3517h int 0Eh

NAMEDITEM 
	PROMPT	"Adapter Memory Location"
	CHOICE  "Segment C800"   pos[1]=XXXX0010b   mem 0c8000h-0cbfffh
	CHOICE  "Segment CC00"   pos[1]=XXXX0011b   mem 0cc000h-0cffffh
	CHOICE  "Segment D000"   pos[1]=XXXX0100b   mem 0d0000h-0d3fffh
	CHOICE  "Segment D400"   pos[1]=XXXX0101b   mem 0d4000h-0d7fffh
	CHOICE  "Segment D800"   pos[1]=XXXX0110b   mem 0d8000h-0dbfffh
	CHOICE  "Segment DC00"   pos[1]=XXXX0111b   mem 0dc000h-0dffffh
	CHOICE  "ROM disabled"   pos[1]=XXXX1XXXb
	HELP
	   "To configure this adapter you must choose the memory 
location the adapter will use for its BIOS ROM. There are seven 
memory locations that can be selected.  Under normal circumstances, 
select <Segment C800>."

	
NAMEDITEM 
	PROMPT	"DMA Arbitration Level"
	CHOICE  "Level_5"   pos[0]=XX0101XXb   arb 5
	CHOICE  "Level_6"   pos[0]=XX0110XXb   arb 6
	CHOICE  "Level_7"   pos[0]=XX0111XXb   arb 7
	CHOICE  "Level_0"   pos[0]=XX0000XXb   arb 0
	CHOICE  "Level_1"   pos[0]=XX0001XXb   arb 1
	CHOICE  "Level_3"   pos[0]=XX0011XXb   arb 3
	CHOICE  "Level_4"   pos[0]=XX0100XXb   arb 4
	HELP
	   "This selects the arbitration priority level the adapter 
will use to transfer data.  Under normal circumstances, select <Level 5>."


NAMEDITEM 
	PROMPT	"DMA Burst Length"
	CHOICE  "8 Word Burst"   pos[1]=XX01XXXXb
	CHOICE  "16 Word Burst"   pos[1]=XX10XXXXb
	CHOICE  "24 Word Burst"   pos[1]=XX11XXXXb
	CHOICE  "Burst Disabled"   pos[1]=XX00XXXXb
	HELP
	   "DMA transfer burst length.  This is the maximum number of 
words that the adapter will transfer in a single DMA transfer.  Under 
normal circumstances, select <8 Word Burst>."


NAMEDITEM 
	PROMPT	"Fairness"
	CHOICE  "On"   pos[0]=X1XXXXXXb
	CHOICE  "Off"  pos[0]=X0XXXXXXb
	HELP
	   "Bus Arbitration Fairness.  This controls whether the 
adapter will release control of the bus when it has been using it 
exclusively.  Under normal circumstances, select <On>."


