
AdapterId 6BBBh

AdapterName "BARR/6BBB Synchronous Communications Adapter from Barr Systems"

NumBytes 2

NamedItem

Prompt "Device Address"
	choice "280-287"  pos[0]=XXXXX00Xb  io 0280h-0287h
	choice "290-297"  pos[0]=XXXXX01Xb  io 0290h-0297h
	choice "2A0-2A7"  pos[0]=XXXXX10Xb  io 02A0h-02A7h
	choice "2B0-2B7"  pos[0]=XXXXX11Xb  io 02B0h-02B7h

Help
"The Device Address can be choosen from: 
     280-287,290-297,2A0-2A7, or 2B0-2B7.
Use the F5=Previous and the F6=Next keys to change this choice.
Conflicting device addresses are marked with an asterisk and
must be changed to use the adapter."



NamedItem

Prompt "Interrupt Request Level"
      choice "IRQ10"    pos[0]=XXX01XXXb  int 10
      choice "IRQ11"    pos[0]=XXX10XXXb  int 11
      choice "IRQ12"    pos[0]=XXX11XXXb  int 12
      choice "IRQ9"     pos[0]=XXX00XXXb  int 9 2

Help
"The Interrupt Request Level can be choosen from: IRQ10,IRQ11,IRQ12,IRQ9.
Use the F5=Previous and the F6=Next keys to change this choice.
Conflicting Interrupt Request Levels must be changed to use the adapter."



NamedItem

Prompt "DMA Channel A Arbitration Level"
      choice "ARB 1"      pos[0]=001XXXXXb  arb 1
      choice "ARB 2"      pos[0]=010XXXXXb  arb 2
      choice "ARB 3"      pos[0]=011XXXXXb  arb 3
      choice "ARB 5"      pos[0]=101XXXXXb  arb 5
      choice "ARB 6"      pos[0]=110XXXXXb  arb 6
      choice "ARB 7"      pos[0]=111XXXXXb  arb 7
      choice "ARB 0"      pos[0]=000XXXXXb  arb 0
      choice "ARB 4"      pos[0]=100XXXXXb  arb 4

Help
"The DMA Channel A Arbitration Level can be choosen from: 1,2,3,5,6,7,0,4.
Use the F5=Previous and the F6=Next keys to change this choice.
Conflicting Arbitration Levels are marked with an asterisk and must be
changed to use the adapter."



NamedItem

Prompt "DMA Channel B Arbitration Level"
      choice "ARB 1"      pos[1]=00100000b  arb 1
      choice "ARB 2"      pos[1]=01000000b  arb 2
      choice "ARB 3"      pos[1]=01100000b  arb 3
      choice "ARB 5"      pos[1]=10100000b  arb 5
      choice "ARB 6"      pos[1]=11000000b  arb 6
      choice "ARB 7"      pos[1]=11100000b  arb 7
      choice "ARB 0"      pos[1]=00000000b  arb 0
      choice "ARB 4"      pos[1]=10000000b  arb 4

Help
"The DMA Channel B Arbitration Level can be choosen from: 1,2,3,5,6,7,0,4.
Use the F5=Previous and the F6=Next keys to change this choice.
Conflicting Arbitration Levels are marked with an asterisk and
must be changed to use the adapter."

