;******************************************************************************
;*                        Tiara Computer Systems, Inc.                        *
;*                             2700 Garcia Avenue                             *
;*                          Mountain View, CA  94043                          *
;*                   LANcard/E-2 Adapter Configuration File                   *
;*                         Tiara Part # 70-00578-0000                         *
;*									      *
;*	Date: 05-16-90							      *
;*									      *
;*	Source File: @6001.ADF						      *
;*	Engineer: Don Stone 						      *
;*									      *
;******************************************************************************

adapterid 06001h

adaptername "Tiara LanCard/E*MC TWISTED PAIR Adapter"

numbytes 4

fixedresources		pos[3]=110XXXXXb

nameditem

	prompt "Base I/O Port Address Select"

	choice "Base I/O Port 1200"	pos[0]=0000XXXXb    io 1200h-121Fh
	choice "Base I/O Port 1220"	pos[0]=0001XXXXb    io 1220h-123Fh
	choice "Base I/O Port 1240"	pos[0]=0010XXXXb    io 1240h-125Fh
	choice "Base I/O Port 1260"	pos[0]=0011XXXXb    io 1260h-127Fh
	choice "Base I/O Port 1280"	pos[0]=0100XXXXb    io 1280h-129Fh
	choice "Base I/O Port 12A0"	pos[0]=0101XXXXb    io 12A0h-12BFh
	choice "Base I/O Port 12C0"	pos[0]=0110XXXXb    io 12C0h-12DFh
	choice "Base I/O Port 12E0"	pos[0]=0111XXXXb    io 12E0h-12FFh
	choice "Base I/O Port 1300"	pos[0]=1000XXXXb    io 1300h-131Fh
	choice "Base I/O Port 1320"	pos[0]=1001XXXXb    io 1320h-133Fh
	choice "Base I/O Port 1340"	pos[0]=1010XXXXb    io 1340h-135Fh
	choice "Base I/O Port 1360"	pos[0]=1011XXXXb    io 1360h-137Fh
	choice "Base I/O Port 1380"	pos[0]=1100XXXXb    io 1380h-139Fh
	choice "Base I/O Port 13A0"	pos[0]=1101XXXXb    io 13A0h-13BFh
	choice "Base I/O Port 13C0"	pos[0]=1110XXXXb    io 13C0h-13DFh
	choice "Base I/O Port 13E0"	pos[0]=1111XXXXb    io 13E0h-13FFh

help

"To configure this adapter, a base I/O port address must be selected.
The default port address is 1200.

Use the F5=Previous and F6=Next keys to change this assignment.
Conflicting assignments are marked with an asterisk and must be changed."




nameditem

	prompt "Interrupt Request Select"

	choice "Interrupt Request IRQ3"	  pos[0]=XXXX00XXb    int 3
	choice "Interrupt Request IRQ4"	  pos[0]=XXXX01XXb    int 4
	choice "Interrupt Request IRQ7"	  pos[0]=XXXX10XXb    int 7
	choice "Interrupt Request IRQ9"	  pos[0]=XXXX11XXb    int 9


help

"To configure this adapter, an interrupt request must be selected.
The default setting is IRQ3.

Use the F5=Previous and F6=Next keys to change this assignment.
Conflicting assignments ARE NOT marked with an asterisk and must be changed."


nameditem

	prompt "Boot PROM Starting Address"

	choice "PROM Disabled"      pos[0]=XXXXXX0Xb
	choice "Address C0000"	    pos[3]=XXXX0000b    pos[0]=XXXXXX1Xb    mem 0C0000h-0C1FFFh
	choice "Address C2000"	    pos[3]=XXXX0001b    pos[0]=XXXXXX1Xb    mem 0C2000h-0C3FFFh
	choice "Address C4000"	    pos[3]=XXXX0010b    pos[0]=XXXXXX1Xb    mem 0C4000h-0C5FFFh
	choice "Address C6000"	    pos[3]=XXXX0011b    pos[0]=XXXXXX1Xb    mem 0C6000h-0C7FFFh
	choice "Address C8000"	    pos[3]=XXXX0100b    pos[0]=XXXXXX1Xb    mem 0C8000h-0C9FFFh
	choice "Address CA000"	    pos[3]=XXXX0101b    pos[0]=XXXXXX1Xb    mem 0CA000h-0CBFFFh
	choice "Address CC000"	    pos[3]=XXXX0110b    pos[0]=XXXXXX1Xb    mem 0CC000h-0CDFFFh
	choice "Address CE000"	    pos[3]=XXXX0111b    pos[0]=XXXXXX1Xb    mem 0CE000h-0CFFFFh
	choice "Address D0000"	    pos[3]=XXXX1000b    pos[0]=XXXXXX1Xb    mem 0D0000h-0D1FFFh
	choice "Address D2000"	    pos[3]=XXXX1001b    pos[0]=XXXXXX1Xb    mem 0D2000h-0D3FFFh
	choice "Address D4000"	    pos[3]=XXXX1010b    pos[0]=XXXXXX1Xb    mem 0D4000h-0D5FFFh
	choice "Address D6000"	    pos[3]=XXXX1011b    pos[0]=XXXXXX1Xb    mem 0D6000h-0D7FFFh
	choice "Address D8000"	    pos[3]=XXXX1100b    pos[0]=XXXXXX1Xb    mem 0D8000h-0D9FFFh
	choice "Address DA000"	    pos[3]=XXXX1101b    pos[0]=XXXXXX1Xb    mem 0DA000h-0DBFFFh
	choice "Address DC000"	    pos[3]=XXXX1110b    pos[0]=XXXXXX1Xb    mem 0DC000h-0DDFFFh
	choice "Address DE000"	    pos[3]=XXXX1111b    pos[0]=XXXXXX1Xb    mem 0DE000h-0DFFFFh

help

"To configure this adapter, a starting address must be selected for the Boot
PROM - if so equipped. The default setting is PROM Disabled and is used if 
there is no boot PROM on the adapter board or to remove the PROM  from the 
computer's memory address space. Otherwise, choose a starting address of C0000.

Use the F5=Previous and F6=Next keys to change this assignment.
Conflicting assignments are marked with an asterisk and must be changed."























































































