;***************************************************************************
;*
;* Copyright (C) 1989-1993 by NCR Corporation.
;*
;* This program contains proprietary and confidential information.
;* All rights reserved except as may be permitted by prior written consent.
;*
;*************************************************************************** 

AdapterId 01BAh

AdapterName "NCR 53C710 SCSI Controller"

NumBytes 4

FixedResources
    pos[0]=XX1XXXXXb
    pos[1]=XXX0XXX0b
    pos[3]=110XXX1Xb

NamedItem
    Prompt "SCSI Controller"
    Choice "Enabled"        pos[0]=XXXXXXX1b
    Choice "Disabled"       pos[0]=XXXXXXX0b
    Help
"This option will allow you to disable the SCSI controller.  Once the
controller is disabled, no SCSI devices connected to this controller can be
accessed after the next system boot."


NamedItem
    Prompt "Memory Address Range"
    Choice "DC000h-DFFFFh"  pos[1]=111XXXXXb mem 0DC000h-0DFFFFh
    Choice "D8000h-DBFFFh"  pos[1]=110XXXXXb mem 0D8000h-0DBFFFh
    Choice "D4000h-D7FFFh"  pos[1]=101XXXXXb mem 0D4000h-0D7FFFh
    Choice "D0000h-D3FFFh"  pos[1]=100XXXXXb mem 0D0000h-0D3FFFh
    Choice "CC000h-CFFFFh"  pos[1]=011XXXXXb mem 0CC000h-0CFFFFh
    Choice "C8000h-CBFFFh"  pos[1]=010XXXXXb mem 0C8000h-0CBFFFh
    Choice "C4000h-C7FFFh"  pos[1]=001XXXXXb mem 0C4000h-0C7FFFh
    Choice "C0000h-C3FFFh"  pos[1]=000XXXXXb mem 0C0000h-0C3FFFh









    Help
"Set the Memory Address Range to avoid conflict with adapters which 
use the Channel ROM area for ROM or RAM."




NamedItem
    Prompt "Interrupt Level"
    Choice "14"             pos[0]=11XXXXXXb int 14
    Choice "11"             pos[0]=10XXXXXXb int 11
    Choice "5"              pos[0]=01XXXXXXb int 5
    Choice "3"              pos[0]=00XXXXXXb int 3
    Help
"Choose an Interrupt Level.  Shared interrupts may degrade system performance."



NamedItem
    Prompt "Arbitration Level"
    Choice "14"             pos[0]=XXX1110Xb arb 14
    Choice "13"             pos[0]=XXX1101Xb arb 13
    Choice "12"             pos[0]=XXX1100Xb arb 12
    Choice "11"             pos[0]=XXX1011Xb arb 11
    Choice "10"             pos[0]=XXX1010Xb arb 10
    Choice "9"              pos[0]=XXX1001Xb arb 9
    Choice "8"              pos[0]=XXX1000Xb arb 8
    Choice "7"              pos[0]=XXX0111Xb arb 7
    Choice "6"              pos[0]=XXX0110Xb arb 6
    Choice "5"              pos[0]=XXX0101Xb arb 5
    Choice "4"              pos[0]=XXX0100Xb arb 4
    Choice "3"              pos[0]=XXX0011Xb arb 3
    Choice "2"              pos[0]=XXX0010Xb arb 2
    Choice "1"              pos[0]=XXX0001Xb arb 1
    Choice "0"              pos[0]=XXX0000Xb arb 0

    Help
"The SCSI Adapter supports the direct memory access mode of data 
transfer.  Each Arbitration level has a corresponding priority level; 
the lower the Arbitration level, the higher the corresponding priority. 
The first level listed is recommended."






NamedItem
    Prompt "Fairness"
    Choice "Enabled"        pos[3]=XXXXXXX0b
    Choice "Disabled"       pos[3]=XXXXXXX1b
    Help
"This option, if 'Enabled', causes the SCSI controller to not compete
for the Micro Channel during the next arbitration phase if it is currently
in control of the Micro Channel.  This allows adapters to obtain the 
Micro Channel in the next sequence based on each adapter's assigned 
priority level.  When 'Disabled', the controller will compete for every 
arbitration phase and will obtain more than its fair share of Micro Channel 
usage.  It is recommended to set Fairness to 'Enabled.'"




NamedItem
    Prompt "I/O Address Range"
    Choice "0800h-08FFh"    pos[2]=000010XXb io 00800h-008FFh
    Choice "0C00h-0CFFh"    pos[2]=000011XXb io 00C00h-00CFFh
    Choice "1000h-10FFh"    pos[2]=000100XXb io 01000h-010FFh
    Choice "1400h-14FFh"    pos[2]=000101XXb io 01400h-014FFh
    Choice "1800h-18FFh"    pos[2]=000110XXb io 01800h-018FFh
    Choice "1C00h-1CFFh"    pos[2]=000111XXb io 01C00h-01CFFh
    Choice "2000h-20FFh"    pos[2]=001000XXb io 02000h-020FFh
    Choice "2400h-24FFh"    pos[2]=001001XXb io 02400h-024FFh
    Choice "2800h-28FFh"    pos[2]=001010XXb io 02800h-028FFh
    Choice "2C00h-2CFFh"    pos[2]=001011XXb io 02C00h-02CFFh
    Choice "3000h-30FFh"    pos[2]=001100XXb io 03000h-030FFh
    Choice "3400h-34FFh"    pos[2]=001101XXb io 03400h-034FFh
    Choice "3800h-38FFh"    pos[2]=001110XXb io 03800h-038FFh
    Choice "3C00h-3CFFh"    pos[2]=001111XXb io 03C00h-03CFFh
    Choice "4000h-40FFh"    pos[2]=010000XXb io 04000h-040FFh
    Choice "4400h-44FFh"    pos[2]=010001XXb io 04400h-044FFh
    Choice "4800h-48FFh"    pos[2]=010010XXb io 04800h-048FFh
    Choice "4C00h-4CFFh"    pos[2]=010011XXb io 04C00h-04CFFh
    Choice "5000h-50FFh"    pos[2]=010100XXb io 05000h-050FFh
    Help
"Choose one of the available I/O Address Range options."





NamedItem
    Prompt "Channel A Host Logical ID"
    Choice "7"              pos[1]=XXXX111Xb
    Choice "6"              pos[1]=XXXX110Xb
    Choice "5"              pos[1]=XXXX101Xb
    Choice "4"              pos[1]=XXXX100Xb
    Choice "3"              pos[1]=XXXX011Xb
    Choice "2"              pos[1]=XXXX010Xb
    Choice "1"              pos[1]=XXXX001Xb
    Choice "0"              pos[1]=XXXX000Xb
    Help
"Set the Logical ID to avoid conflict when performing I/O with other 
SCSI devices.  The default is 7.  This may be the same as the 'Channel B
Host Logical ID' since channel A and channel B are on separate physical
SCSI buses."

NamedItem
    Prompt "Channel B Host Logical ID"
    Choice "7"              pos[3]=XXX111XXb
    Choice "6"              pos[3]=XXX110XXb
    Choice "5"              pos[3]=XXX101XXb
    Choice "4"              pos[3]=XXX100XXb
    Choice "3"              pos[3]=XXX011XXb
    Choice "2"              pos[3]=XXX010XXb
    Choice "1"              pos[3]=XXX001XXb
    Choice "0"              pos[3]=XXX000XXb
    Help
"Set the Logical ID to avoid conflict when performing I/O with other 
SCSI devices.  The default is 7.  This may be the same as the 'Channel A
Host Logical ID' since channel A and channel B are on seperate physical
SCSI buses.  This option is only active if there is a Daughter Card attached."

NamedItem
    Prompt "Controller Priority"
    Choice "Equal"                          pos[2]=XXXXXXX1b
    Choice "Channel A"                      pos[2]=XXXXXX10b
    Choice "Channel B"                      pos[2]=XXXXXX00b
    Help
"The controllers on each SCSI Bus will take turns accessing the Micro 
Channel if this option is set to 'Equal'.  If the 'Channel A' or 'Channel B'
controller has priority, that controller will always win when the two 
controllers compete for the Micro Channel."
