AdapterId 06FE6h

AdapterName "DigiBoard PS-COM/4"

NumBytes 1

NamedItem

Prompt "UART Address Range"

choice "0x5B40 -> 0x5B60"
	      pos[0]=xxxx000xb
	      io 05b40h-05b60h
choice "0x4B40 -> 0x4B60"
	      pos[0]=xxxx001xb
	      io 04b40h-04b60h
choice "0x3B40 -> 0x3B60"
	      pos[0]=xxxx010xb
	      io 03b40h-03b60h
choice "0x2B40 -> 0x2B60"
	      pos[0]=xxxx011xb
	      io 02b40h-02b60h
choice "0x5B00 -> 0x5B20"
	      pos[0]=xxxx100xb
	      io 05b00h-05b20h
choice "0x4B00 -> 0x4B20"
	      pos[0]=xxxx101xb
	      io 04b00h-04b20h
choice "0x3B00 -> 0x3B20"
	      pos[0]=xxxx110xb
	      io 03b00h-03b20h


Help

"No Help Available"


NamedItem

Prompt "Com2 Status"

choice "Disabled"
	      pos[0]=0xxxxxxxb
choice "Enabled"
	      pos[0]=1xxxxxxxb
	      io 02f8h-02ffh
Help

"No help is Available"

NamedItem

Prompt "Interrupt Select"

choice "INT 3" pos[0]=x000xxxxb   int 3
choice "INT 4" pos[0]=x001xxxxb   int 4
choice "INT 5" pos[0]=x010xxxxb   int 5
choice "INT 7" pos[0]=x011xxxxb   int 7
choice "INT 10" pos[0]=x100xxxxb  int 10
choice "INT 11" pos[0]=x101xxxxb  int 11
choice "INT 12" pos[0]=x110xxxxb  int 12
choice "INT 15" pos[0]=x111xxxxb  int 15

Help

"No Help is currently available"
