
AdapterId 0678dh

AdapterName  "NeoTecH MSP/4, 4 channel serial + parallel adapter "

NumBytes 1

NamedItem
        Prompt "Serial_n/Parallel_n"       
  choice "Serial_2-5,parallel_2"  pos[0]=XXXX0001b  io 0378h-037fh
                                                       02F8h-02ffh  
                                                       3220h-3227h
                                                       3228h-322fh
                                                       4220h-4227h int 3 7
  choice "Serial_2-5,parallel_3"  pos[0]=XXXX0011b  io 0278h-027fh
                                                       02F8h-02ffh  
                                                       3220h-3227h
                                                       3228h-322fh
                                                       4220h-4227h int 3 7
  choice "Serial_2-5,no parallel"  pos[0]=XXXX0101b io 02F8h-02ffh  
                                                       3220h-3227h
                                                       3228h-322fh
                                                       4220h-4227h int 3
  choice "Serial_2-5,parallel_1"  pos[0]=XXXX1101b  io 03BCh-03Bfh
                                                       02F8h-02ffh  
                                                       3220h-3227h
                                                       3228h-322fh
                                                       4220h-4227h int 3 7
  choice "Serial_6-9,parallel_2"  pos[0]=XXXX0111b  io 0378h-037fh
                                                       4228h-422fh
                                                       5220h-5227h
                                                       5228h-522fh  
                                                       6220h-6227h int 3 7
  choice "Serial_6-9,parallel_3"  pos[0]=XXXX1001b  io 0278h-027fh
                                                       4228h-422fh
                                                       5220h-5227h
                                                       5228h-522fh  
                                                       6220h-6227h int 3 7
  choice "Serial_6-9,no parallel"  pos[0]=XXXX1011b io 4228h-422fh
                                                       5220h-5227h
                                                       5228h-522fh  
                                                       6220h-6227h int 3 
  choice "Serial_6-9,parallel_1"  pos[0]=XXXX1111b  io 03BCh-03Bfh
                                                       4228h-422fh
                                                       5220h-5227h
                                                       5228h-522fh  
                                                       6220h-6227h int 3 7

 Help
"This allows you to set the SERIAL and PARALLEL ports to the desired
 configuration. LPT assignments are determined by the BIOS POST function
 and do not necessarily correspond to the PARALLEL port assignments.
 PS/2 models 80-A21 and 80-A31 differ from most PS/2's. For more
 information remove the MSP/4, return to your operating system, insert
 the installation diskette and type LPTINFO <enter>."
