AdapterId 07052h

AdapterName  "AST RampagePlus/MC With I/O Pak/MC-SP Option"

NumBytes 4

NamedItem
   Prompt "Wait State"
      choice "1 wait state " pos[1]=0XXXXXXXb
      choice "0 wait state " pos[1]=1XXXXXXXb
   Help
      "Memory WAIT STATE selection"

NamedItem
   Prompt "Memory Configuration"
      choice "DISABLED"   pos[0]=1010000Xb
      choice ".5M,0K,0K,0K    TOTAL = 0.5 MB" pos[0]=1111001Xb
      choice ".5M,.5M,0K,0K   TOTAL = 1.0 MB" pos[0]=1110001Xb
      choice ".5M,.5M,.5M,0K  TOTAL = 1.5 MB" pos[0]=1101001Xb
      choice ".5M,.5M,.5M,.5M TOTAL = 2.0 MB" pos[0]=1100001Xb
      choice " 2M,0K,0K,0K    TOTAL = 2.0 MB" pos[0]=1001001Xb
      choice ".5M,2M,0K,0K    TOTAL = 2.5 MB" pos[0]=0110001Xb
      choice ".5M,.5M,2M,0K   TOTAL = 3.0 MB" pos[0]=0101001Xb
      choice ".5M,.5M,.5M,2M  TOTAL = 3.5 MB" pos[0]=0100001Xb
      choice " 2M,2M,0K,0K    TOTAL = 4.0 MB" pos[0]=1000001Xb
      choice ".5M,2M,2M,0K    TOTAL = 4.5 MB" pos[0]=0011001Xb
      choice ".5M,.5M,2M,2M   TOTAL = 5.0 MB" pos[0]=0111001Xb
      choice " 2M,2M,2M,0K    TOTAL = 6.0 MB" pos[0]=0001001Xb
      choice ".5M,2M,2M,2M    TOTAL = 6.5 MB" pos[0]=0010001Xb
      choice " 2M,2M,2M,2M    TOTAL = 8.0 MB" pos[0]=0000001Xb
   Help
"This is memory configuration on your RampagePlus/MC
starting from top of the board BANK0,BANK1,BANK2,BANK3"

NamedItem
     Prompt "Connector 1"
      choice "SERIAL_1"
                       pos[2]=xxxx0001b
                       io 03f8h-03ffh int 4
      choice "SERIAL_2"
                       pos[2]=xxxx0011b
                       io 02f8h-02ffh int 3
      choice "SERIAL_3"
                       pos[2]=xxxx0101b
                       io 3220h-3227h int 3
      choice "SERIAL_4"
                       pos[2]=xxxx0111b
                       io 3228h-322fh int 3
      choice "SERIAL_5"
                       pos[2]=xxxx1001b
                       io 4220h-4227h int 3
      choice "SERIAL_6"
                       pos[2]=xxxx1011b
                       io 4228h-422fh int 3
      choice "SERIAL_7"
                       pos[2]=xxxx1101b
                       io 5220h-5227h int 3
      choice "SERIAL_8"
                       pos[2]=xxxx1111b
                       io 5228h-522fh int 3
      choice "DISABLE"
                       pos[2]=xxxxxxx0b
   Help
      "Connector 1 of RampagePlus/MC Serial and Parallel Port
      Option can have  any one of the  Serial 1  to  Serial 8
      assignments  and  can  also  be  disabled.  Use the F5=
      Previous and the F6=Next keys to change the Connector 1
      Serial port assignments  when  you  are  in the 'Change
      Configuration'  window.   Conflicting  assignments  are
      marked with an Asterisk and should be changed."

NamedItem
   Prompt "Connector 2"
      choice "PARALLEL_1" pos[2]=xx01xxxxb io 03bch-03bfh int 7
      choice "PARALLEL_2" pos[2]=xx10xxxxb io 0378h-037fh int 7
      choice "PARALLEL_3" pos[2]=xx11xxxxb io 0278h-027fh int 5
      choice "DISABLE"    pos[2]=xx00xxxxb
   Help
      "Connector 2 of the RampagePlus/MC  Serial and Parallel
      Port Option can  have  any  one  of  the  Parallel 1 to
      Parallel 3 assignments and can  also  be disabled.  Use
      the  F5=Previous  and  the F6=Next  keys  to change the
      Connector 2 Parallel Port  assignments  when you are in
      the 'Change Configuration' window.   Conflicting assig-
      nments  are  marked  with  an  Asterisk  and  should be
      changed."
