
AdapterId 062FFh

AdapterName "The Quadram MainLink IIM - 3270 Connection"

NumBytes 3

FixedResources
         pos[0]=XXXXXXXXb
         io 0220h-022Fh 02D0h-02DFh
         int 2

NamedItem

    Prompt "Adapter BIOS ROM Location"
         Choice "Segment CC00"
              pos[2]=1X000110b
              mem 0CC000h-0CFFFFh
         Choice "Segment D000"
              pos[2]=1X001000b
              mem 0CE000h-0D1FFFh
         Choice "Segment D200"
              pos[2]=1X001001b
              mem 0CE000h-0CFFFFh 0D2000h-0D3FFFh
         Choice "Segment D400"
              pos[2]=1X001010b
              mem 0CE000h-0CFFFFh 0D4000h-0D5FFFh
         Choice "Segment D600"
              pos[2]=1X001011b
              mem 0CE000h-0CFFFFh 0D6000h-0D7FFFh
         Choice "Segment D800"
              pos[2]=1X001100b
              mem 0CE000h-0CFFFFh 0D8000h-0D9FFFh
         Choice "Segment DA00"
              pos[2]=1X001101b
              mem 0CE000h-0CFFFFh 0DA000h-0DBFFFh
         Choice "Segment DC00"
              pos[2]=1X001110b
              mem 0CE000h-0CFFFFh 0DC000h-0DDFFFh
         Choice "Segment DE00"
              pos[2]=1X001111b
              mem 0CE000h-0CFFFFh 0DE000h-0DFFFFh
         Choice "ROM Disabled"
              pos[2]=0X001000b
              mem 0CE000h-0CFFFFh

    Help
         "To configure this adapter, you must choose the memory location
         that the adapter will use for it's BIOS ROM.  There are 10
         locations that can be selected.  Under normal circumstances,
         the default selection, <Segment CC00>, is adequate."

