
AdapterID 0FDDEh

AdapterName "Enhanced 80386 Memory Expansion Adapter w/ROM"

Numbytes 4

FixedResources
  POS[0]=0xxxx011b
  POS[1]=xxxxxxxxb
  POS[2]=xxxxxxxxb
  POS[3]=11xxxxxxb Exec


NamedItem Prompt "ROM Address Range"
          Choice  "C8000-C9FFF"  pos[0]=x0100xxxb  mem 0C8000h - 0C9FFFh
          Choice  "CA000-CBFFF"  pos[0]=x0101xxxb  mem 0CA000h - 0CBFFFh
          Choice  "CC000-CDFFF"  pos[0]=x0110xxxb  mem 0CC000h - 0CDFFFh
          Choice  "CE000-CFFFF"  pos[0]=x0111xxxb  mem 0CE000h - 0CFFFFh
          Choice  "D0000-D1FFF"  pos[0]=x1000xxxb  mem 0D0000h - 0D1FFFh
          Choice  "D2000-D3FFF"  pos[0]=x1001xxxb  mem 0D2000h - 0D3FFFh
          Choice  "D4000-D5FFF"  pos[0]=x1010xxxb  mem 0D4000h - 0D5FFFh
          Choice  "D6000-D7FFF"  pos[0]=x1011xxxb  mem 0D6000h - 0D7FFFh
          Choice  "D8000-D9FFF"  pos[0]=x1100xxxb  mem 0D8000h - 0D9FFFh
          Choice  "DA000-DBFFF"  pos[0]=x1101xxxb  mem 0DA000h - 0DBFFFh
          Choice  "DC000-DDFFF"  pos[0]=x1110xxxb  mem 0DC000h - 0DDFFFh
          Choice  "DE000-DFFFF"  pos[0]=x1111xxxb  mem 0DE000h - 0DFFFFh
          Choice  "Disabled" pos[0]=x0000xxxb
          Help
          "This assignment need only be changed if it is in conflict
           with another card.  Conflicting assignments are marked
           with an asterisk. If there are multiple Enhanced 80386
           Memory Expansion Adapters w/ROM installed in the system,
           only one is required to have a ROM address. The other
           Enhanced Adapters can have the Rom Address Range set to
           Disabled by using the Change Configuration utility."

NamedItem Prompt "Enabled Memory"
          Choice  "Run Set Configuration"   pos[3]=xx111111b
          Choice  "0KB (0MB)"         pos[3]=xx000000b
          Choice  "1024KB (1.0MB)"    pos[3]=xx000001b
          Choice  "2048KB (2.0MB)"    pos[3]=xx000010b
          Choice  "3072KB (3.0MB)"    pos[3]=xx000011b
          Choice  "4096KB (4.0MB)"    pos[3]=xx000100b
          Choice  "5120KB (5.0MB)"    pos[3]=xx000101b
          Choice  "6144KB (6.0MB)"    pos[3]=xx000110b
          Choice  "7168KB (7.0MB)"    pos[3]=xx000111b
          Choice  "8192KB (8.0MB)"    pos[3]=xx001000b
          Choice  "9216KB (9.0MB)"    pos[3]=xx001001b
          Choice  "10240KB (10.0MB)"  pos[3]=xx001010b
          Choice  "11264KB (11.0MB)"  pos[3]=xx001011b
          Choice  "12288KB (12.0MB)"  pos[3]=xx001100b
          Choice  "13312KB (13.0MB)"  pos[3]=xx001101b
          Choice  "14336KB (14.0MB)"  pos[3]=xx001110b
          Choice  "15360KB (15.0MB)"  pos[3]=xx001111b
          Choice  "16384KB (16.0MB)"  pos[3]=xx010000b
          Help
          "This item is used to allow the amount of enabled memory
           on the memory card to be displayed when the configuration
           is viewed. Modifying this field does not affect the amount
           of enabled memory on the memory card.

           This entry shows the amount of memory that can be enabled
           on the adapter. Since the total system memory cannot exceed
           16 megs, some of this memory may not be enabled.

           If 'Run Set Configuration' appears in the display,
           Set Configuration must be run again to re-display
           the amount of enabled memory."




