; file @67E1.ADF used to configure the
; Extended TTY 8 Port Controller Card


AdapterId       067e1h

AdapterName     "NCR  8 Port Serial Controller/MC"

NumBytes        4

NamedItem
Prompt  "Dual Port Address"
choice "0d0000H" pos[0]=xxx0000xb pos[1]=11010000b MEM 0d0000h-0d1fffh
choice "0d2000H" pos[0]=xxx0000xb pos[1]=11010010b MEM 0d2000h-0d3fffh
choice "0d4000H" pos[0]=xxx0000xb pos[1]=11010100b MEM 0d4000h-0d5fffh
choice "0d6000H" pos[0]=xxx0000xb pos[1]=11010110b MEM 0d6000h-0d7fffh
choice "0d8000H" pos[0]=xxx0000xb pos[1]=11011000b MEM 0d8000h-0d9fffh
choice "0da000H" pos[0]=xxx0000xb pos[1]=11011010b MEM 0da000h-0dbfffh
choice "0dc000H" pos[0]=xxx0000xb pos[1]=11011100b MEM 0dc000h-0ddfffh
choice "0de000H" pos[0]=xxx0000xb pos[1]=11011110b MEM 0de000h-0dffffh
Help
"This selects the address of the dual port memory.
 The dual port address may be set on any 8k byte
 boundary.  Under normal circumstances, select 0d0000H.
 Use the F5=Previous and the F6=Next keys to change this
 assignment.  Conflicting assignments are marked with an
 asterisk and must be changed to use the adapter."



NamedItem
Prompt "Enable Interrupts"
choice "Enabled " pos[3]=110x1xxxb
choice "Disabled" pos[3]=110x0xxxb
Help
"This item enables or disables the controller to interrupt
the host. When enabled, the controller will interrupt the
host on the IRQ level specified by the 'INTERRUPT LEVEL'
item.  Default condition is interrupts enabled."


NamedItem
Prompt "Interrupt Level"
choice "IRQ 3 " pos[3]=xxxxx000b  INT 3
choice "IRQ 4 " pos[3]=xxxxx001b  INT 4
choice "IRQ 5 " pos[3]=xxxxx010b  INT 5
choice "IRQ 7 " pos[3]=xxxxx011b  INT 7
choice "IRQ 9 " pos[3]=xxxxx100b  INT 9
choice "IRQ 10" pos[3]=xxxxx101b  INT 10
choice "IRQ 11" pos[3]=xxxxx110b  INT 11
choice "IRQ 12" pos[3]=xxxxx111b  INT 12
Help
"This item specifies at which IRQ level the controller will
interrupt the host.  When enabled via the 'ENABLE INTERRUPTS'
item, the controller will interupt the host on the level
specified here. Ensure the selected IRQ level does not
conflict with another device."
 

;end of file

