AdapterID 0425h

AdapterName "SUPERFAX MODEM ADAPTOR"

NumBytes 4

fixedresources
        pos[0]=00000001b
        pos[1]=00000XXXb
        pos[2]=00000XXXb
        pos[3]=000XXXXXb

nameditem
        Prompt  "FAX MODEM BASE IO Address Location"
          Choice "Address Segment 2000h INT 7"
            pos[1]=XXXXX000b	
	    pos[2]=XXXXX000b
            io 2000h-201Fh    	
	    int 7
          Choice "Address Segment 2400h INT 9"
            pos[1]=XXXXX001b	 
            pos[2]=XXXXX001b
            io 2400h-241Fh  
	    int 9
          Choice "Address Segment 2800h INT 10"
            pos[1]=XXXXX010b
	    pos[2]=XXXXX010b
            io 2800h-281Fh  
	    int 10
          Choice "Address Segment 2C00h INT 11"
            pos[1]=XXXXX011b		      
	    pos[2]=XXXXX011b
            io 2C00h-2C1Fh  
	    int 11
          Choice "Address Segment 3000h INT 3"
            pos[1]=XXXXX100b		     
	    pos[2]=XXXXX100b
            io 3000h-301Fh  
	    int 3
          Choice "Address Segment 3400h INT 4"
            pos[1]=XXXXX101b
	    pos[2]=XXXXX101b
            io 3400h-341Fh		     
	    int 4
          Choice "Address Segment 3800h INT 5"
            pos[1]=XXXXX110b
	    pos[2]=XXXXX110b
            io 3800h-381Fh
	    int 5
          Choice "Address Segment 3C00h INT 6"
            pos[1]=XXXXX111b
	    pos[2]=XXXXX111b
            io 3C00h-3C1Fh
	    int 6

        Help
        "There are eight possible address assigments in the interrupt 
	 and I/O space area for the FAX Modem Adaptor.  The addressing 
	 range for each address segment is 4 byte.  The start addresses
         (interrupt) for the eight possible combinations are 2000h(7), 
	 2400h(9), 2800h(10), 2C00(11), 3000(3), 3400(4), 3800(5), 3C00(6).  
	 Use F5 = Previous and the F6 = Next keys to change address 
	 selection.  Under normal situation, select <Segment 2000h>."


nameditem
        Prompt  "DMA Arbitration Level Selection"
          Choice  "Level 1"
            pos[3]=XXXX0001b
            arb 1
          Choice  "Level 2"
            pos[3]=XXXX0010b
            arb 2
          Choice  "Level 3"
            pos[3]=XXXX0011b
            arb 3
          Choice  "Level 5"
            pos[3]=XXXX0101b
            arb 5
          Choice  "Level 6"
            pos[3]=XXXX0110b
            arb 6
          Choice  "Level 7"
            pos[3]=XXXX0111b
            arb 7
          Choice  "Level 8"
            pos[3]=XXXX1000b
            arb 8
          Choice  "Level 9"
            pos[3]=XXXX1001b
            arb 9
          Choice  "Level 10"
            pos[3]=XXXX1010b
            arb 10
          Choice  "Level 11"
            pos[3]=XXXX1011b
            arb 11
          Choice  "Level 12"
            pos[3]=XXXX1100b
            arb 12
          Choice  "Level 13"
            pos[3]=XXXX1101b
            arb 13
          Choice  "Level 14"
            pos[3]=XXXX1110b
            arb 14
        Help
        "This assignment need only be changed if it is in conflict
         with another assigment.  Conflicting assigments are marked
         with an asterisk.  Use the F5 = Previous and the F6 = Next
         keys to change arbitration level assigments.  Using arbitration
         levels, this adapter accesses memory directly without
         burdening the computer's main processor.  An aribitration
         level of 0 has the highest priority, and increasing levels
         have the corresponing decreased priority.  Under normal
         situation, select <Level 1>."

nameditem
        Prompt  "DMA Fairness"
          Choice  "On"
            pos[3]=XXX1XXXXb
          Choice  "Off"
            pos[3]=XXX0XXXXb
        Help
        "The Fairness allows the system to service all arbitrating
         devices on the Micro channel in order of priority before
         the same device can gain control of the Micro-channel again.
         Under normal situation, select <DMA Fairness On>"
