; Torus Ethernet Adapter/MC
; Adapter Description File
;
; Version:   1.01a
;
; (C) Copyright Torus Systems Ltd. 1987


AdapterID 06BFFh

AdapterName "Torus Ethernet Adapter/MC"

NumBytes 2

FixedResources
     POS[0]=0XXXXX1Xb


NamedItem Prompt "Memory Address Range"

  Choice "D0000 - D7FFF"
     POS[1]=100XXXXXb
     MEM 0D0000h - 0D7FFFh

  Choice "D4000 - DBFFF"
     POS[1]=101XXXXXb
     MEM 0D4000h - 0DBFFFh

  Choice "D8000 - DFFFF"
     POS[1]=110XXXXXb
     MEM 0D8000h - 0DFFFFh

  Choice "C0000 - C7FFF"
     POS[1]=000XXXXXb
     MEM 0C0000h - 0C7FFFh

  Choice "C4000 - CBFFF"
     POS[1]=001XXXXXb
     MEM 0C4000h - 0CBFFFh

  Choice "C8000 - CFFFF"
     POS[1]=010XXXXXb
     MEM 0C8000h - 0CFFFFh

  Choice "CC000 - D3FFF"
     POS[1]=011XXXXXb
     MEM 0CC000h - 0D3FFFh

  Help "MEMORY ADDRESS RANGE:  There are 7 possible 32 Kbyte address ranges      
        which can be assigned to access the memory located on the Torus
        Ethernet Adapter.  The default memory address range for the adapter
        is D0000 - D7FFF.  The assigned memory address range can be changed
        by selecting 'Change Configuration' and then using the F5=Previous 
        and the F6=Next keys.  The address range selected must not be  
        assigned for use by any other adapter or option.  If an assignment
        has an asterisk (*) by it, it is in conflict with another assignment 
        and the memory address range must be changed.  If a conflict 
        remains, you may have to change the assignments for other adapters
        or options that are in your computer to resolve the conflict."


NamedItem Prompt "I/O Address Range"

  Choice "0300 - 031F"
     POS[1]=XXX000XXb
     IO  0300h - 031Fh

  Choice "0320 - 033F"
     POS[1]=XXX001XXb
     IO  0320h - 033Fh

  Choice "0400 - 041F"
     POS[1]=XXX010XXb
     IO  0400h - 041Fh

  Choice "0420 - 043F"
     POS[1]=XXX011XXb
     IO  0420h - 043Fh

  Choice "0500 - 051F"
     POS[1]=XXX100XXb
     IO  0500h - 051Fh

  Choice "0520 - 053F"
     POS[1]=XXX101XXb
     IO  0520h - 053Fh

  Choice "0600 - 061F"
     POS[1]=XXX110XXb
     IO  0600h - 061Fh

  Help "I/O ADDRESS RANGE:  There are 7 possible 16 byte I/O address ranges 
        which can be assigned to access the Torus Ethernet Adapter.
        The default I/O address range for the adapter is 0300 - 031F.
        The assigned I/O address range can be changed by selecting 
        'Change Configuration' and then using the F5=Previous and the
        F6=Next keys.  The I/O address range selected must not be assigned
        for use by any other adapter or option.  If an assignment has an
        asterisk (*) by it, it is in conflict with another assignment 
        and the I/O address range must be changed.  If a conflict remains,
        you may have to change the assignments for other adapters or 
        options that are in your computer to resolve the conflict ."



NamedItem Prompt "Interrupt Request Line (IRQ)"
 
  Choice "IRQ 3"
     POS[1]=XXXXXX00b
     INT 3d
 
  Choice "IRQ 5"
     POS[1]=XXXXXX01b
     INT 5d
 
  Choice "IRQ 10"
     POS[1]=XXXXXX10b
     INT 10d
 
  Choice "IRQ 11"
     POS[1]=XXXXXX11b
     INT 11d
 
  Help "INTERRUPT REQUEST LINE (IRQ):  This Torus Ethernet Adapter can use
        one of four interrupt request lines: 3, 5, 10, or 11.  The default
        interrupt request line is 3.  The assigned interrupt request line
        can be changed by selecting 'Change Configuration' and then using
        the F5=Previous and the F6=Next keys."


  

