
AdapterId 06dedh

AdapterName  "U.S. Robotics Courier 2400 eps"

NumBytes 1

NamedItem
        Prompt "Serial(COM) Address"
      choice "SERIAL_1"  pos[0]=XXXX000Xb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXXX001Xb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXXX010Xb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXXX011Xb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXXX100Xb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXXX101Xb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXXX110Xb  io 5220h-5227h  int 3
      choice "SERIAL_8"  pos[0]=XXXX111Xb  io 5228h-522fh  int 3
   Help
"The Courier 2400eps can be assigned to use Serial 1
through Serial 8.  Use the F5=Previous and the F6=Next
keys to change serial port assignments. Conflicting
assignments are marked with an asterisk. Conflicts
must be resolved to use the adapter."

NamedItem
	Prompt "Smart/Dumb"
     choice "SMART COMMANDS ENABLED" pos[0]=xxx0xxxxb
     choice "DUMB MODEM W/ AUTO ANS" pos[0]=xxx1xxxxb
  Help
"Use this setting to enable or disable the modem's command set.
When set to 'DUMB', the modem cannot originate calls, but will
answer the phone. This could be useful for applications needing 
restricted access to the phone lines. Toggle between the choices
with the F5=Previous or F6=Next keys."


NamedItem
	Prompt "Power-up Defaults"
     choice "BOOT STORED DEFAULTS FROM NVRAM" pos[0]=xx1xxxxxb
     choice "BOOT FACTORY SETTINGS FROM PROM" pos[0]=xx0xxxxxb
  Help
"Use this setting to specify whether the modem uses its 
internal non-volatile memory to initialize its settings
on power-up. Using the FACTORY SETTINGS choice assures 
that the modem is always initialized to known settings,
regardless of previous use. Toggle between the choices
with the F5=Previous or F6=Next keys."

