
;	$Revision:   1.2  $
;	$Date:   26 Jun 1989 11:29:50  $
;
; ***************************************************************************
; * Copyright (C) 1988 by Phoenix Technologies Ltd.  This program           *
; * contains proprietary and confidential information.  All rights reserved *
; * except as may be permitted by prior written consent.                    *
; ***************************************************************************

AdapterId 7511h

AdapterName  "Internal Options"

; This is irrelevant but must be present for the parser
NumBytes 0

; ***********************************************************
NamedItem
        Cmos 0h	MemInst
        Prompt  "Installed memory"
        Choice "16384 KB (16.0 MB)" pos[0]=XXXXXXXXb
        Help
" This is the amount of physically installed memory. It cannot be changed in this
 program."

; ***********************************************************
NamedItem
        Cmos 0h	MemAvail
        Prompt  "Available memory"
        Choice "16384 KB (16.0 MB)" pos[0]=XXXXXXXXb
        Help
" This is the amount of memory that passed parity checking during power-on.
 It cannot be changed in this program."

; ***********************************************************
NamedItem
        Cmos 10h Diskette
        Prompt  "Disk Drive A Type"
        Choice "1.44MB 3.5 Inch" pos[0]=0100XXXXb
	Choice "720KB  3.5 Inch" pos[0]=0011XXXXb
	Choice "360KB 5.25 Inch" pos[0]=0001XXXXb
	Choice "1.2MB 5.25 Inch" pos[0]=0010XXXXb
        Choice "Not Installed"  pos[0]=0000XXXXb
        Help
"Select one of the choices listed for drive A. Use the
F5 (Previous) or F6 (Next) keys to change the drive type."

; ***********************************************************
NamedItem
        Cmos 10h Diskette
        Prompt  "Disk Drive B Type"
        Choice "Not Installed"  pos[0]=XXXX0000b
        Choice "1.44MB 3.5 Inch" pos[0]=XXXX0100b
	Choice "720KB  3.5 Inch" pos[0]=XXXX0011b
	Choice "360KB 5.25 Inch" pos[0]=XXXX0001b
	Choice "1.2MB 5.25 Inch" pos[0]=XXXX0010b
        Help
"Select one of the choices listed for drive B. Use the
F5 (Previous) or F6 (Next) keys to change the drive type."

; ***********************************************************
NamedItem
        Cmos 14h Math
        Prompt "Math Coprocessor"
        Choice "- 80x87 chip -" pos[0]=XXXXXXXXb
        Help
"Your computer has a built in math coprocessor socket to hold a
math coprocessor chip. It cannot be changed prior to its physical installation and
detection."

; ******************************************************************
; Cmos offset 31 (System Board POS 2)
; Bit 3    - 0 = Serial port 1 enabled.
;          - 1 = Serial port 2 enabled.
; Bit 2    - 0 = Serial port disabled.
;          - 1 = Serial port enabled.
; Bit 0    - 0 = Override bits 4,2,1 to disable the ports.
;          - 1 = Enable the state of bits 4,2,1.
; ******************************************************************
NamedItem
        Cmos 31h Board
        Prompt "Serial Port"
        Choice "SERIAL_1"    pos[0]=XXXX1111b io 03f8h-03ffh  int 4
        Choice "SERIAL_2"    pos[0]=XXXX0111b io 02f8h-02ffh  int 3
        Choice "Disabled"    pos[0]=XXXXX011b
        Help
"The built-in serial port can be assigned as Serial port 1,
 Serial port 2, or disabled. Use the F5 (Previous) or F6 (Next) keys to change the
serial port."


; ******************************************************************
; Cmos offset 31 (System Board POS 2)
; Bit 7    - 0 = 8 bit bidrectional mode.
;            1 = bidirectional mode disabled.
; Bit 6,5  - 0,0 = Parallel 1
;          - 0,1 = Parallel 2
;          - 1,0 = Parallel 3
;          - 1,1 = Reserved
; Bit 4    - 0 = Parallel port disabled.
;          - 1 = Parallel port enabled.
; Bit 0    - 0 = Override bits 4,2,1 to disable the ports and diskette.
;          - 1 = Enable the state of bits 4,2,1.
; ******************************************************************
NamedItem
        Cmos 31h
        Prompt "Parallel Port"
        Choice "PARALLEL_1"               pos[0]=1001XX11b io 03bch-03beh int 7
        Choice "PARALLEL_2"               pos[0]=1011XX11b io 0378h-037ah int 7
        Choice "PARALLEL_3"               pos[0]=1101XX11b io 0278h-027ah int 7
        Choice "PARALLEL_1 bidirectional" pos[0]=0001XX11b io 03bch-03beh int 7
        Choice "PARALLEL_2 bidirectional" pos[0]=0011XX11b io 0378h-037ah int 7
        Choice "PARALLEL_3 bidirectional" pos[0]=0101XX11b io 0278h-027ah int 7
        Choice "Disabled"                 pos[0]=XXX0XX11b
        Help
"The built-in parallel port can be assigned as Parallel port 1, 2
 or 3 or disabled entirely. In addition the port can be configured as an
 8-bit bidirectional interface. Use the F5 (Previous) or F6 (Next) keys to
 change the parallel port."

PSignature
NamedItem
        ECmos 703h
        Prompt "System Speed"
        Choice "Fast"                     pos[0]=XXXXXXX0b
        Choice "Slow"                     pos[0]=XXXXXXX1b
        Help
"This option is only valid if your Processor module is equipped with 
Cache, e.g., 486 with internal cache or 386 with external Cache. Choose
one of the speed settings listed, generally <FAST> should be selected
unless you are having problems with applications executing too fast.
Speed definitions are as follows:
     -- Fast ---- Normal Operation with Cache Enabled 
     -- Slow ---- Normal Operation with Cache Disabled
"
; ***********************************************************

PSignature
NamedItem
	ECmos 705h
	Prompt "Internal Imbedded Hard Disk"
	Choice "Enabled"    pos[0]=XXXXXXX1b
	Choice "Disabled"   pos[0]=XXXXXXX0b
	Help
"Choose <Enabled> if you want to use the imbedded hard disk on the mother
board. Else use <Disabled> for any Micro Channel Hard Disk Controller."

PSignature
NamedItem
	ECmos 706h
	Prompt 	"Interrupt Level"
	Choice 	"INT 14"    pos[0]=XXXXXXX0b	  int 14
	Choice 	"INT 15"    pos[0]=XXXXXXX1b	  int 15
	Help
"If the Internal Hard Drive is enabled, you must choose the interrupt level 
for the drive to interrupt the system. Default condition is <INT 14>. This
option is ignored if the Internal Hard Drive is not selected."

PSignature
NamedItem
	ECmos 706h
	Prompt   "Adapter I/O Address"
	Choice   "I/O Address 01F0h-01FFh"    pos[0]=XXXXX00Xb    io 01F0h-01FFh
	Choice   "I/O Address 11F0h-11FFh"    pos[0]=XXXXX01Xb    io 11F0h-11FFh
	Choice   "I/O Address 21F0h-21FFh"    pos[0]=XXXXX10Xb    io 21F0h-21FFh
	Choice   "I/O Address 31F0h-31FFh"    pos[0]=XXXXX11Xb    io 31F0h-31FFh
	Help
"If the Internal Hard Drive is enabled, you must choose the I/O location 
for the drive to interface to the system. There are four possible I/O spaces.
Under normal circumstances, select <I/O Address 01F0h-01FFh>. This option
is ignored if the Internal Hard Drive is not selected."

PSignature
NamedItem
	ECmos 706h
	Prompt   "Automatic Insertion of AT Drive Type"
	Choice   "No"     pos[0]=XXXX0XXXb
	Choice   "Yes"    pos[0]=XXXX1XXXb
	Help
"If the Internal Hard Drive is selected and you choose to run Xenix or Novell, 
you must enable the Automatic Insertion of Drive Type for the device drivers
under these two Operating Systems to recognize the drive. For others OS, 
Automatic Insertion is not needed."


PSignature
NamedItem
	ECmos 704h
	Prompt "Maximum Memory Limit"
	Choice "No Limit"	pos[0]=XXXXXXX0b
	Choice "16 MB Limit"	pos[0]=XXXXXXX1b
	Help
"Chose <No Limit> unless you are running which does not recognize memory
above the 16MB boundry."

; Reserve a group of resources for the system board
FixedResources NoDisplay
	pos[0]=xxxxxxxxb

; DMA, Keyboard, CMOS/NMI, Math Coproc, Interrupt Controller, etc
        IO 01h-0108h
; Video
        IO 03c0h-03dfh
; Diskette
        IO 03f0h-03f7h

; Diskette Arbitration
        ARB 2
