;Rev. 01 06/30/93

AdapterId 06795h

AdapterName " NeoTecH Single RS-422/485 Async. Adapter, S1M200"

NumBytes 3

NamedItem
        Prompt "Port Address"
        
        choice "SERIAL_2 (02f8h)" pos[1]=11111XXXb
                                  pos[2]=00000010b  io 02f8h-02ffh 
        
        choice "SERIAL_3 (3220h)" pos[1]=00100XXXb
                                  pos[2]=00110010b  io 3220h-3227h 
        
        choice "SERIAL_4 (3228h)" pos[1]=00101XXXb
                                  pos[2]=00110010b  io 3228h-322fh 
        
        choice "SERIAL_5 (4220h)" pos[1]=00100XXXb
                                  pos[2]=01000010b  io 4220h-4227h 
        
        choice "SERIAL_6 (4228h)" pos[1]=00101XXXb
                                  pos[2]=01000010b  io 4228h-422fh 
        
        choice "SERIAL_7 (5220h)" pos[1]=00100XXXb
                                  pos[2]=01010010b  io 5220h-5228h
        
        choice "SERIAL_8 (5228h)" pos[1]=00101XXXb
                                  pos[2]=01010010b  io 5228h-522fh 
        
        choice "SERIAL_1 (03f8h)" pos[1]=11111XXXb
                                  pos[2]=00000011b  io 03f8h-03ffh 

Help
"This port can be assigned to Serial 1-8. Use F5=Previous and the 
F6=Next keys to change serial port assignments if you are in the 'Change 
configuration' window. Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."

NamedItem
        Prompt "Interrupt Level"
        
        choice "Int 3" pos[0]=XXXXX11Xb  int 3
        
        choice "Int 4" pos[0]=XXXXX10Xb  int 4
        
        choice "Int 7" pos[0]=XXXXX01Xb  int 7  
        
        choice "Int 9" pos[0]=XXXXX00Xb  int 9  

Help
"This port can be assigned to Interrupt level 3, 4, 7, or 9. Use 
F5=Previous and the F6=Next keys to change serial port assignments if you are 
in the 'Change configuration' window. Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."

NamedItem
        Prompt "Transmitter Driver Control"
        
        choice "RS-422 (always enabled)" pos[0]=XXX11XXXb
        
        choice "RS-485 (enabled by RTS)" pos[0]=XXX01XXXb
        
        choice "RS-485 (enabled by DTR)" pos[0]=XXX10XXXb
        
        choice "Always DISABLED        " pos[0]=XXX00XXXb

Help
"This port may be defined as RS-422 or RS-485.  RS-422 is most commonly used
in a four wire, full duplex mode (2 devices).  RS-485 is used in a two or 
four wire half duplex mode with a 'bus' type architecture.  Either the DTR 
signal or RTS signal may be used to control the line drivers.  Use 
F5=Previous and the F6=Next keys to change serial port assignments if you are 
in the 'Change configuration' window."
