AdapterId 0613Fh

AdapterName "SONIC Model 50,60,70,80 Demo Board"

NumBytes 2

FixedResources 
	pos[0]= xxxx0xxxb
	pos[1]= xxxxxxx0b

nameditem
        Prompt  "Adapter - IO Location"
          Choice "0x0400-0x04ff"
            pos[0]=0000xxxxb
            io 0400h-04ffh
           Choice "0x1e00-0x1eff"
            pos[0]=1101xxxxb
            io 1e00h-1effh
          Choice "0x1c00-1cff0x"
            pos[0]=1100xxxxb
            io 1c00h-1cffh
          Choice "0x1a00-1aff0x"
            pos[0]=1011xxxxb
            io 1a00h-1affh
          Choice "0x1800-18ff0x"
            pos[0]=1010xxxxb
            io 1800h-18ffh
          Choice "0x1600-16ff0x"
            pos[0]=1001xxxxb
            io 1600h-16ffh
          Choice "0x1400-0x14ff"
            pos[0]=1000xxxxb
            io 1400h-14ffh
          Choice "0x1200-0x12ff"
            pos[0]=0111xxxxb
            io 1200h-12ffh
          Choice "0x1000-0x1000"
            pos[0]=0110xxxxb
            io 1000h-1000h
          Choice "0x0e00-0x0eff"
            pos[0]=0101xxxxb
            io 0e00h-0effh
          Choice "0x0c00-0x0cff"
            pos[0]=0100xxxxb
            io 0c00h-0cffh
          Choice "0x0a00-0x0aff"
            pos[0]=0011xxxxb
            io 0a00h-0affh
          Choice "0x0800-0x08ff"
            pos[0]=0010xxxxb
            io 0800h-08ffh
          Choice "0x0600-0x06ff"
            pos[0]=0001xxxxb
            io 0600h-06ffh
       Help
	"There are 14 i/o location can be selected."

nameditem
        Prompt  "Select Thick or Thin wire Ethernet"
          Choice  "Thin wire Ethernet"
            pos[1]=xxxxx0xxb
          Choice  "Thick wire Ethernet"
            pos[1]=xxxxx1xxb
Help
	"This bit selects the thin or thick wire ethernet. The
	 default choice is thin-Ethernet"

nameditem
	Prompt	"Interrupt Request number"
	  Choice  "IRQ 3"
	    pos[0]=xxxxx00xb
	    int 3
	  Choice  "IRQ 6"
	    pos[0]=xxxxx01xb
	    int 6
	  Choice  "IRQ 7"
	    pos[0]=xxxxx10xb
	    int 7
	  Choice  "IRQ 9"
	    pos[0]=xxxxx11xb
	    int 9
        Help
        "The SONIC EB uses one interrupt for signalling the CPU.
	 There are four possible interrupts to choose from. For
	 normal installations IRQ 9 should be selected."


nameditem
	Prompt "Arbitration Level"
  	Choice "Level 0"
	  pos[1]=0000xxxxb
	  arb 0

  	Choice "Level 14"
	  pos[1]=1110xxxxb
	  arb 14

  	Choice "Level 13"
	  pos[1]=1101xxxxb
	  arb 13

  	Choice "Level 12"
	  pos[1]=1100xxxxb
	  arb 12

  	Choice "Level 11"
	  pos[1]=1011xxxxb
	  arb 11

  	Choice "Level 10"
	  pos[1]=1010xxxxb
	  arb 10

  	Choice "Level 9"
	  pos[1]=1001xxxxb
	  arb 9

  	Choice "Level 8"
	  pos[1]=1000xxxxb
	  arb 8

  	Choice "Level 7"
	  pos[1]=0111xxxxb
	  arb 7

  	Choice "Level 6"
	  pos[1]=0110xxxxb
	  arb 6

  	Choice "Level 5"
	  pos[1]=0101xxxxb
	  arb 5

  	Choice "Level 4"
	  pos[1]=0100xxxxb
	  arb 4

  	Choice "Level 3"
	  pos[1]=0011xxxxb
	  arb 3

  	Choice "Level 2"
	  pos[1]=0010xxxxb
	  arb 2

  	Choice "Level 1"
	  pos[1]=0001xxxxb
	  arb 1


Help
	"There are 14 arbitration levels. The default will be 
	 ARB0. "



nameditem
	Prompt "Select Fairness Enable"
	  Choice "Fairness Enable"
		pos[1]=xxxx1xxxb

	  Choice "Fairness Disable"
		pos[1]=xxxx0xxxb

Help
	"The default for the fairness enable bit is 1."

nameditem
	Prompt "Select Internal/External ENDEC"
	  Choice "Internal SONIC ENDEC Enabled"
		pos[1]=xxxxxx0xb

	  Choice "Internal ENDEC disabled"
		pos[1]=xxxxxx1xb

Help
	"This bit allows the internal ENDEC to be enabled or disabled."

