
AdapterID 0568Dh

AdapterName  "MaynStream SCSI Tape Adapter"

NumBytes 2

nameditem
     Prompt  "Adapter Address"
        Choice "FF70H to FF77H" pos[0]=XXXXX10Xb io 0ff70h-0ff77h
        Choice "FF60H to FF67H" pos[0]=XXXXX00Xb io 0ff60h-0ff67h
        Help
        "The MaynStream SCSI Tape Adapter can reside at two different
        I/O Addresses.  Select an address that does not conflict with
        other adapters.  An address conflict is indicated by an
        asterisk."


nameditem
     Prompt  "DMA Arbitration Levels"
        Choice  "Level 5"  pos[0]=010XXXXXb  arb 5
        Choice  "Level 1"  pos[0]=110XXXXXb  arb 1
        Choice  "Level 3"  pos[0]=100XXXXXb  arb 3
        Choice  "Level 4"  pos[0]=011XXXXXb  arb 4
        Choice  "Level 6"  pos[0]=001XXXXXb  arb 6
        Choice  "Level 7"  pos[0]=000XXXXXb  arb 7
        Choice  "Non-DMA mode" pos[0]=111XXXXXb
        Help
        "The MaynStream SCSI Tape Adapter can support several different DMA
        Arbitration levels.  Select an arbitration level for the MaynStream
        SCSI Tape Adapter that does not conflict with other adapters. An
        arbitration conflict is indicated by an asterisk.  The non-DMA mode
        does not use DMA or interrupts."

nameditem
     Prompt  "Interrupt Level"
        Choice  "Level 2"  pos[0]=XXX00XXXb int 2
        Choice  "Level 3"  pos[0]=XXX01XXXb int 3
        Choice  "Level 5"  pos[0]=XXX10XXXb int 5
        Choice  "Level 7"  pos[0]=XXX11XXXb int 7
        Help
        "The MaynStream SCSI Tape Adapter can support several different
        interrupt levels.  Although it is unnecessary to use an unique
        interrupt, it is recommended that you do so."
