
AdapterId 0EDFFH

AdapterName  "IBM Internal Modem"

NumBytes 1

NamedItem
	Prompt "Serial Configuration"
      choice "SERIAL_1"  pos[0]=XXXX000Xb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXXX001Xb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXXX010Xb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXXX011Xb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXXX100Xb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXXX101Xb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXXX110Xb  io 5220h-5227h  int 3
      choice "SERIAL_8"  pos[0]=XXXX111Xb  io 5228h-522fh  int 3
   Help
"The IBM Internal Modem can be assigned to use Serial 1
through Serial 8.  Use the F5=Previous and the F6=Next
keys to change serial port assignments.  Conflicting
assignments are marked with an asterisk and must be
changed."


