;Cypress/2 TOKEN RING Configuration Diskette Program
;Lantana Technology Inc. 
;File @0F2F.adf
;version 1.0 rev A      01/03/89 

AdapterID 00F2Fh

AdapterName  "Lantana Technology Cypress/2 Token Ring MCA."

NumBytes 3

nameditem
        Prompt  "Daughter Board enable"
          Choice "Enable  " pos[0]=1XXXXXXXb
          Choice "Disable " pos[0]=0XXXXXXXb
        Help
         "Enable if Daughter Board is present"
nameditem
        Prompt  "Burned-In Address Enable"
          Choice "Enable  " pos[0]=X1XXXXXXb
          Choice "Disable " pos[0]=X0XXXXXXb
        Help
         " This option must be Enable at all times"


nameditem
        Prompt  "I/O Port Address Range"
          Choice "0A20-0A2F" pos[2]=XXXXXXX1b io 0A20h-0A2Fh
          Choice "1A20-1A2F" pos[2]=XXXXXXX0b io 1A20h-1A2Fh
        Help
         "I/O PORT ADDRESS RANGE                               
         Select one of these address ranges for the Cypress/2 
         controller's I/O Ports. Be sure that the address range 
         that you select has not been used by any other expansion
         card (a conflict is indicated by an asterisk)."

nameditem
        Prompt  "Interrupt Level"
          Choice  "IRQ 2 (9)"  pos[2]=XXXX010Xb int 9
          Choice  "IRQ 3"  pos[2]=XXXX011Xb int 3
          Choice  "IRQ 4"  pos[2]=XXXX100Xb int 4
          Choice  "IRQ 5"  pos[2]=XXXX101Xb int 5
          Choice  "IRQ 7"  pos[2]=XXXX111Xb int 7
          Choice  "IRQ 10" pos[2]=XXXX101Xb int 10
          Choice  "None "  pos[2]=XXXX111Xb
        Help
         "INTERRUPT LEVEL                                         
          Select an Interrupt Level for the Cypress/2 Controller.
          It is strongly recommended that  you select an  interrupt
          level that has not been used by any other expansion card."

nameditem
        Prompt  "Arbitration Level"
          Choice  "LEVEL 8 " pos[3]=110X1000b arb 8
          Choice  "LEVEL 9 " pos[3]=110X1001b arb 9
          Choice  "LEVEL 10" pos[3]=110X1010b arb 10
          Choice  "LEVEL 11" pos[3]=110X1011b arb 11
          Choice  "LEVEL 12" pos[3]=110X1100b arb 12
          Choice  "LEVEL 13" pos[3]=110X1101b arb 13
          Choice  "LEVEL 14" pos[3]=110X1110b arb 14
          Choice  "LEVEL 0 " pos[3]=110X0000b arb 0
          Choice  "LEVEL 1 " pos[3]=110X0001b arb 1
          Choice  "LEVEL 2 " pos[3]=110X0010b arb 2
          Choice  "LEVEL 3 " pos[3]=110X0011b arb 3
          Choice  "LEVEL 4 " pos[3]=110X0100b arb 4
          Choice  "LEVEL 5 " pos[3]=110X0101b arb 5
          Choice  "LEVEL 6 " pos[3]=110X0110b arb 6
          Choice  "LEVEL 7 " pos[3]=110X0111b arb 7
        Help
         "ARBITRATION LEVEL                            
          Each Cypress/2 Controller must be assigned a unique
          ARBITRATION LEVEL. Select the level you wish."

nameditem
        Prompt  "Fairness Enable Algorithm"
          Choice  "ENABLE " pos[3]=1101XXXXb
          Choice  "DISABLE" pos[3]=1100XXXXb
        Help
         "Each Cypress/2 Controller must be assigned with the
         fairness enable algoritm enable if you whish allow to 
         all  the  contenders  for  the  bus  to have the same 
         access oportunity. (be fair)."
