
AdapterId 06800h

AdapterName  "Star Gate PLUS 8 MC Adapter"

NumBytes 3

FixedResources
pos[0]=0000000Xb

NamedItem
Prompt "Base I/O Address"
choice "0400H"  pos[1]=00000100b  io 0400h-04ffh
choice "0500H"  pos[1]=00000101b  io 0500h-05ffh
choice "0600H"  pos[1]=00000110b  io 0600h-06ffh
choice "0700H"  pos[1]=00000111b  io 0700h-07ffh
choice "0800H"  pos[1]=00001000b  io 0800h-08ffh
choice "0900H"  pos[1]=00001001b  io 0900h-09ffh
choice "0A00H"  pos[1]=00001010b  io 0a00h-0affh
choice "0B00H"  pos[1]=00001011b  io 0b00h-0bffh
Help
"This selects the Base I/O Address of the UARTS and
Interrupt Status Register.  The adapter uses 256
consecutive I/O ports, starting at the Base I/O Address.
Under normal circumstances, select 0400H.  Use the
F5=Previous and the F6=Next keys to change this
assignment.  Conflicting assignments are marked with an
asterisk and must be changed to use the adapter."

NamedItem
Prompt "Interrupt Level"
choice "IRQ  3"  pos[2]=00000000b  int  3
choice "IRQ  4"  pos[2]=00000001b  int  4
choice "IRQ  5"  pos[2]=00000010b  int  5
choice "IRQ  7"  pos[2]=00000011b  int  7
choice "IRQ  9"  pos[2]=00000100b  int  9
choice "IRQ 10"  pos[2]=00000101b  int 10
choice "IRQ 11"  pos[2]=00000110b  int 11
choice "IRQ 12"  pos[2]=00000111b  int 12
choice "No IRQ"  pos[2]=00001000b
Help
"This selects the Interrupt Level that the UARTS use.
Under normal cicumstances, select IRQ 3.  Use the
F5=Previous and the F6=Next keys to change this
assignment."

