AdapterId 0E1FFh

AdapterName "The IBM 3270 Connection Ver. B/C"

NumBytes 4

FixedResources

         pos[0] = xxxxxxxxb
         pos[3] = 11111010b
         int 2

NamedItem

       Prompt "I/O Address"

       Choice  "02D0-02DF"

         pos[2] = 00000000b
         io 02D0h - 02DFh

       Choice  "06D0-06DF"

         pos[2] = 00000100b
         io 06D0h - 06DFh

       Choice  "0AD0-0ADF"

         pos[2] = 00001000b
         io 0AD0h - 0ADFh

       Choice  "0ED0-0EDF"

         pos[2] = 00001100b
         io 0ED0h - 0EDFh


   Help

      "The First, Second, Third and Fourth choices are available to
      allow up to four adapters in the machine or to resolve conflicts
      with other adapters.  First is the normal choice and matches the
      original adapter's configuration.  The choices can be made by
      selecting the Change Configuration option and using F5=Previous
      and F6=Next keys.  If an assignment has an asterisk (*) by it
      then a conflict exists and either this adapter or the one in
      conflict must be assigned differently."


NamedItem

       Prompt "Memory Assignments"


       Choice  "CE00"

         pos[1] = 11001110b
         mem 0CE000h- 0CFFFFh

       Choice  "CA00"

         pos[1] = 11001010b
         mem 0CA000h- 0CBFFFh

       Choice  "CC00"

         pos[1] = 11001100b
         mem 0CC000h- 0CDFFFh

       Choice  "D000"

         pos[1] = 11010000b
         mem 0D0000h- 0D1FFFh

       Choice  "D200"

         pos[1] = 11010010b
         mem 0D2000h- 0D3FFFh

       Choice  "D400"

         pos[1] = 11010100b
         mem 0D4000h- 0D5FFFh

       Choice  "D600"

         pos[1] = 11010110b
         mem 0D6000h- 0D7FFFh

       Choice  "D800"

         pos[1] = 11011000b
         mem 0D8000h- 0D9FFFh

       Choice  "DA00"

         pos[1] = 11011010b
         mem 0DA000h- 0DBFFFh

       Choice  "DC00"

         pos[1] = 11011100b
         mem 0DC000h- 0DDFFFh

       Choice  "DE00"

         pos[1] = 11011110b
         mem 0DE000h- 0DFFFFh


   Help

      "There are 11 Memory Assignments available when using more than
      one adapter or to resolve conflicts with other adapters.  CE00
      is the normal choice and matches the original adapter's
      configuration.  The choices can be made by selecting the Change
      Configuration option and using F5=Previous and F6=Next keys.  If
      an assignment has an asterisk (*) by it then a conflict exists
      and either this adapter or the one in conflict must be assigned
      differently."
