
AdapterId 06EF8h

AdapterName "IRMA 3t 3270 Coax Adapter"

NumBytes 4 

NamedItem
        Prompt "DCA Emulator Address"

      choice "280h-29Fh"
      pos[0]=xx00x00xb io 0280h-029Fh
      choice "680h-69Fh"
      pos[0]=xx00x01xb io 0680h-069Fh
      choice "A80h-A9Fh"
      pos[0]=xx00x10xb io 0A80h-0A9Fh
      choice "E80h-E9Fh"
      pos[0]=xx00x11xb io 0E80h-0E9Fh
      choice "2A0h-2BFh"
      pos[0]=xx10x00xb io 02A0h-02BFh
      choice "6A0h-6BFh"
      pos[0]=xx10x01xb io 06A0h-06BFh
      choice "AA0h-ABFh"
      pos[0]=xx10x10xb io 0AA0h-0ABFh
      choice "EA0h-EBFh"
      pos[0]=xx10x11xb io 0EA0h-0EBFh
      choice "2C0h-2DFh"
      pos[0]=xx01x00xb io 02C0h-02DFh
      choice "6C0h-6DFh"
      pos[0]=xx01x01xb io 06C0h-06DFh
      choice "AC0h-ADFh"
      pos[0]=xx01x10xb io 0AC0h-0ADFh
      choice "EC0h-EDFh"
      pos[0]=xx01x11xb io 0EC0h-0EDFh
      choice "6E0h-6FFh"
      pos[0]=xx11x01xb io 06E0h-06FFh
      choice "AE0h-AFFh"
      pos[0]=xx11x10xb io 0AE0h-0AFFh
      choice "EE0h-EFFh"
      pos[0]=xx11x11xb io 0EE0h-0EFFh

   Help

      "This is the DCA Emulator Address. There are 15 choices available.
       If you choose XC0H, disable the IBM interface to avoid IO 
       conflicts. 
       If the DCA Emulator Address conflicts with another adapter board
       in the PC you can :
       1. Change the Port Address setting on the other board to resolve 
          the conflict or 
       2. Choose one of the alternate addresses and reconfigure
          the DCA Emulator Address."

NamedItem
        Prompt "IRMA Emulator Port Address"
          Choice  "Enable 220-227"  
        pos[2] = x11xx1xxb io 0220h-0227h
          Choice  "Disable 220-227"  
        pos[2] = x11xx0xxb 

   Help

          "The IRMA Emulator port Address is fixed at 220h. If the IRMA 
      Emulator Port Address conflicts with another adapter board in the PC 
      you can: 
      1. Change the Port Address setting on the other board to resolve the 
         conflict or 
      2. Choose 'Disable 220 - 227'. Older DCA emulation software, such as 
         E78, and applications written for the original PROM board IRMA 
         product only run at address 220 - 227. If your software requires 
         this address 'Enable 220 - 227' must be selected. Current DCA 
         emulators, i.e. E78 PLUS, Irmax - Multisession and Irmax - DFT, can 
         be configured to use the DCA Emulator addresses selected above."

NamedItem
        Prompt "IRQ level or Disable Interrupt"
          Choice "IRQ2 "   pos[1]=xxx11000b int 2
          Choice "IRQ10"   pos[1]=xxx11001b int 10
          Choice "Disable INT"  pos[1]=xxx0xxxxb

   Help

      "When using IBM emulation software or DCA Irmax - DFT or 
      Irmax - Multisessions, IRQ2 (same as IRQ9) must be selected."

NamedItem
        Prompt "IBM Emulator Port Address"
          choice "2D0h-2DFh"
          pos[0]=xxxxx00xb pos[1]=xxx11000b pos[2]=x11xxx11b io 02D0h - 02DFh int 2
          choice "6D0h-6DFh"
          pos[0]=xxxxx01xb pos[1]=xxx11000b pos[2]=x11xxx11b io 06D0h - 06DFh int 2
          choice "AD0h-ADFh"
          pos[0]=xxxxx10xb pos[1]=xxx11000b pos[2]=x11xxx11b io 0AD0h - 0ADFh int 2
          choice "ED0h-EDFh"
          pos[0]=xxxxx11xb pos[1]=xxx11000b pos[2]=x11xxx11b io 0ED0h - 0EDFh int 2

          choice "Disable IBM"
          pos[0]=xxxxxxxxb pos[2]=x11xxx0xb

   Help

      "Choose 02D0h - 02DFH if IRMA 3 Emulator Address setting is configured
      at 2XX range.  
      Choose 06D0h - 06DFH if IRMA 3 Emulator Address setting is configured
      at 6XX range.  
      Choose 0AD0h - 0ADFH if IRMA 3 Emulator Address setting is configured
      at AXX range.  
      Choose 0ED0h - 0EDFH if IRMA 3 Emulator Address setting is configured
      at EXX range.  
      If these resources conflict with another adapter board in the PC
      you can: 
      1. Change the resource requirements on the other board to resolve
         the conflict or
      2. Choose one of the four alternate addresses and reconfigure
         DCA Emulator Address or
      3. Choose 'Disable IBM'. You can not run IBM emulation software
         on IRMA 3 if IBM is disabled."

NamedItem
        Prompt "RAM Address Range"
         choice "CE000 - CFFFF"
             pos[2]=x11xxxx1b pos[3]=10x0111xb MEM 0CE000h - 0CFFFFh
         choice "CC000 - CDFFF"
             pos[2]=x11xxxx1b pos[3]=10x0110xb MEM 0CC000h - 0CDFFFh
         choice "CA000 - CBFFF"
             pos[2]=x11xxxx1b pos[3]=10x0101xb MEM 0CA000h - 0CBFFFh
         choice "C8000 - C9FFF"
             pos[2]=x11xxxx1b pos[3]=10x0100xb MEM 0C8000h - 0C9FFFh
         choice "C6000 - C7FFF"
             pos[2]=x11xxxx1b pos[3]=10x0011xb MEM 0C6000h - 0C7FFFh
         choice "C4000 - C5FFF"
             pos[2]=x11xxxx1b pos[3]=10x0010xb MEM 0C4000h - 0C5FFFh
         choice "C2000 - C3FFF"
             pos[2]=x11xxxx1b pos[3]=10x0001xb MEM 0C2000h - 0C3FFFh
         choice "C0000 - C1FFF"
             pos[2]=x11xxxx1b pos[3]=10x0000xb MEM 0C0000h - 0C1FFFh
         choice "D0000 - D1FFF"
             pos[2]=x11xxxx1b pos[3]=10x1000xb MEM 0D0000h - 0D1FFFh
         choice "D2000 - D3FFF"
             pos[2]=x11xxxx1b pos[3]=10x1001xb MEM 0D2000h - 0D3FFFh
         choice "D4000 - D5FFF"
             pos[2]=x11xxxx1b pos[3]=10x1010xb MEM 0D4000h - 0D5FFFh
         choice "D6000 - D7FFF"
             pos[2]=x11xxxx1b pos[3]=10x1011xb MEM 0D6000h - 0D7FFFh
         choice "D8000 - D9FFF"
             pos[2]=x11xxxx1b pos[3]=10x1100xb MEM 0D8000h - 0D9FFFh
         choice "DA000 - DBFFF"
             pos[2]=x11xxxx1b pos[3]=10x1101xb MEM 0DA000h - 0DBFFFh
         choice "DC000 - DDFFF"
             pos[2]=x11xxxx1b pos[3]=10x1110xb MEM 0DC000h - 0DDFFFh
         choice "DE000 - DFFFF"
             pos[2]=x11xxxx1b pos[3]=10x1111xb MEM 0DE000h - 0DFFFFh
         choice "Disable RAM"
               pos[2]=x11xxxx0b pos[3]=10x0000xb

   Help

      "When using IBM emulation software Ram Address Range must
      be selected. If the Ram Address Range conflicts with another 
      adapter in the PC you can : 
      1. Change the Ram Address setting on the other board to
         resolve the conflict or  
      2. Choose one of the sixteen memory addresses and configure
         the DCA emulator to use the new address or  
      3. Choose 'Disable Ram'. You can not run IBM emulation
         software on IRMA 3 if Disable Ram is selected."

