
AdapterId 0EFDFh

AdapterName  "ARCNET controller: ASTER/2 "

NumBytes 1

NamedItem

        Prompt "Base Port and Mem Location, Int Level"

        choice "Port 2e0, Mem 0D000, Int 2"

                pos[0] = 0010000Xb
                io 02E0h - 02EFh
                int 2
                mem 0D0000h - 0D7FFFh


        choice "Port 2e0, Mem 0D800, Int 2"

                pos[0] = 0011000Xb
                io 02E0h - 02EFh
                int 2
                mem 0D8000h - 0DFFFFh

        choice "Port 2f0, Mem 0D000, Int 2"

                pos[0] = 0110000Xb
                io 02F0h - 02FFh
                int 2
                mem 0D0000h - 0D7FFFh

        choice "Port 2f0, Mem 0D800, Int 2"

                pos[0] = 0111000Xb
                io 02F0h - 02FFh
                int 2
                mem 0D8000h - 0DFFFFh

        choice "Port 300, Mem 0D000, Int 2"

                pos[0] = 1010000Xb
                io 0300h - 030Fh
                int 2
                mem 0D0000h - 0D7FFFh

        choice "Port 300, Mem 0D800, Int 2"

                pos[0] = 1011000Xb
                io 0300h - 030Fh
                int 2
                mem 0D8000h - 0DFFFFh

        choice "Port 2e0, Mem 0C000, Int 2"

                pos[0] = 0000000Xb
                io 02E0h - 02EFh
                int 2
                mem 0C0000h - 0C7FFFh

        choice "Port 2e0, Mem 0C800, Int 2"

                pos[0] = 0001000Xb
                io 02E0h - 02EFh
                int 2
                mem 0C8000h - 0CFFFFh

        choice "Port 2f0, Mem 0C000, Int 2"

                pos[0] = 0100000Xb
                io 02F0h - 02FFh
                int 2
                mem 0C0000h - 0C7FFFh

        choice "Port 2f0, Mem 0C800, Int 2"

                pos[0] = 0101000Xb
                io 02F0h - 02FFh
                int 2
                mem 0C8000h - 0CFFFFh

        choice "Port 300, Mem 0C000, Int 2"

                pos[0] = 1000000Xb
                io 0300h - 030Fh
                int 2
                mem 0C0000h - 0C7FFFh

        choice "Port 300, Mem 0C800, Int 2"

                pos[0] = 1001000Xb
                io 0300h - 030Fh
                int 2
                mem 0C8000h - 0CFFFFh

        choice "Port 2e0, Mem 0D000, Int 3"

                pos[0] = 0010001Xb
                io 02E0h - 02EFh
                int 3
                mem 0D0000h - 0D7FFFh

        choice "Port 2f0, Mem 0D000, Int 3"

                pos[0] = 0110001Xb
                io 02F0h - 02FFh
                int 3
                mem 0D0000h - 0D7FFFh

        choice "Port 2e0, Mem 0D000, Int 4"

                pos[0] = 0010010Xb
                io 02E0h - 02EFh
                int 4
                mem 0D0000h - 0D7FFFh

        choice "Port 2f0, Mem 0D000, Int 4"

                pos[0] = 0110010Xb
                io 02F0h - 02FFh
                int 4
                mem 0D0000h - 0D7FFFh




  Help

"To configure this adapter you may choose the base port address,
base memory location, and interrupt level. The base port number
is the first port address that is used. The base memory address
is where the first addressable memory location is found. This is
the shareable memory that is contained within the network 
controller. The interrupt levels are used to interrupt the host
processor when data is recieved through the network.
Use the F5=Previous and the F6=Next keys to change this
assignment. Conflicting assignments are marked with an asterisk
and must be changed."

