
AdapterID 0EFF5h

AdapterName  "Ungermann-Bass NICps/2 Ethernet LAN Adapter"

NumBytes 4

nameditem
	Prompt "Enable/Disable Adapter"
	  Choice  "Adapter Enabled"
		pos[0]=XXXXXXX1b
		int 03h
	  Choice  "Adapter Disabled"
		pos[0]=XXXXXXX0b
	Help
	"This controls whether the adapter is enabled or not.  Under normal
	 circumstances, select <Adapter Enabled>."

nameditem
	Prompt	"RAM Memory Address Range"
	  Choice "D0000 - D7FFF"
		pos[1]=00001101b
		pos[3]=1X10XX00b
		mem 0d0000h-0d7fffh
	  Choice "D8000 - DFFFF"
		pos[1]=00001101b
		pos[3]=1X10XX10b
		mem 0d8000h-0dffffh
	  Choice "C0000 - C7FFF"
		pos[1]=00001100b
		pos[3]=1X10XX00b
		mem 0c0000h-0c7fffh
	  Choice "C8000 - CFFFF"
		pos[1]=00001100b
		pos[3]=1X10XX10b
		mem 0c8000h-0cffffh
	Help
	"To configure this adapter you must choose the range of memory
	 addresses the adapter will use for its 32 KB of RAM.  There are
	 four ranges that can be selected.  Under normal circumstances,
	 select <D0000 - D7FFF>."

nameditem
	Prompt	"ROM Memory Address Range"
	  Choice "C0000 - C3FFF"
		pos[2]=00001100b
		pos[3]=10XX00XXb
		mem 0c0000h-0c3fffh
	  Choice "C4000 - C7FFF"
		pos[2]=00001100b
		pos[3]=10XX01XXb
		mem 0c4000h-0c7fffh
	  Choice "C8000 - CBFFF"
		pos[2]=00001100b
		pos[3]=10XX10XXb
		mem 0c8000h-0cbfffh
	  Choice "CC000 - CFFFF"
		pos[2]=00001100b
		pos[3]=10XX11XXb
		mem 0cc000h-0cffffh
	  Choice "D0000 - D3FFF"
		pos[2]=00001101b
		pos[3]=10XX00XXb
		mem 0d0000h-0d3fffh
	  Choice "D4000 - D7FFF"
		pos[2]=00001101b
		pos[3]=10XX01XXb
		mem 0d4000h-0d7fffh
	  Choice "D8000 - DBFFF"
		pos[2]=00001101b
		pos[3]=10XX10XXb
		mem 0d8000h-0dbfffh
	  Choice "DC000 - DFFFF"
		pos[2]=00001101b
		pos[3]=10XX11XXb
		mem 0dc000h-0dffffh
	Help
	"To configure this adapter you must choose the range of memory
	 addresses the adapter will use for its 16 KB of EPROM.  There
	 are eight ranges that can be selected.  Under normal circumstances,
	 select <C0000 - C3FFF>."

nameditem
	Prompt	"I/O Port Address Range"
	  Choice "1550h - 1553h"
		pos[0]=xxxx100xb
		io 1550h - 1553h
	  Choice "1554h - 1557h"
		pos[0]=xxxx101xb
		io 1554h - 1557h
	  Choice "1558h - 155Bh"
		pos[0]=xxxx110xb
		io 1558h - 155Bh
	  Choice "155Ch - 155Fh"
		pos[0]=xxxx111xb
		io 155Ch - 155Fh
	Help
	"To configure this adapter you must choose the range of I/O addresses
	 the adapter will use for its 4 I/O ports.  There are four ranges
	 that can be selected. Under normal circumstances, select
	 <1550h - 1553h>."

nameditem
	Prompt	"Adapter Timer Interval"
	  Choice  "65.536 milliseconds"
		pos[0]=11XXXXXXb
	  Choice  "32.768 milliseconds"
		pos[0]=10XXXXXXb
	  Choice  "16.384 milliseconds"
		pos[0]=01XXXXXXb
	  Choice  " 8.192 milliseconds"
		pos[0]=00XXXXXXb
	Help
	"This selects the interval at which the adapter's timer will operate.
	 Under normal circumstances, select <65.536 milliseconds>."

