
;
; IBM TTL Async Adapter description File
; Version:      1.00
;
; (C) Copyright International Business Machines Corporation 1988
; All rights reserved.
;

AdapterID 0EFF8H

AdapterName  "TTL Async Adapter"

NumBytes 1

NamedItem
      Prompt "TTL Async communication board"
      choice "TTL Async 1"  pos[0]=XXXXX00Xb  io 04F8h-04FFh  int 3
      choice "TTL Async 2"  pos[0]=XXXXX01Xb  io 0CF8h-0CFFh  int 3

   Help
      "To configure this adapter you must choose the port
      address. There are two addresses that can be selected.
      <TTL Async 1> is preferred, but the adapter can
      operate on any of the two addresses.
      Use the F5=Previous and F6=Next keys to change this
      assignment. Conflicting assignments are marked with
      an asterisk and must be changed."

