
AdapterID 062F0h

AdapterName  "Plexus AIP2 Card"

NumBytes 4

fixedresources
	pos[3]=XX0XXXXXb

nameditem
	Prompt	"Adapter Memory Location"
	  Choice  "Segment C400"
            pos[0]=XXXXXX1Xb
            pos[1]=11000XXXb
	    mem 0c4000h-0c7fffh

	  Choice  "Segment C800"
            pos[0]=XXXXXX0Xb
            pos[1]=11001XXXb
	    mem 0c8000h-0cbfffh

	  Choice  "Segment CC00"
            pos[0]=XXXXXX1Xb
            pos[1]=11001XXXb
	    mem 0cc000h-0cffffh

	  Choice  "Segment D000"
            pos[0]=XXXXXX0Xb
            pos[1]=11010XXXb
	    mem 0d0000h-0d3fffh

	  Choice  "Segment D400"
            pos[0]=XXXXXX1Xb
            pos[1]=11010XXXb
	    mem 0d4000h-0d7fffh

	  Choice  "Segment D800"
            pos[0]=XXXXXX0Xb
            pos[1]=11011XXXb
	    mem 0d8000h-0dbfffh

	  Choice  "Segment DC00"
            pos[0]=XXXXXX1Xb
            pos[1]=11011XXXb
	    mem 0dc000h-0dffffh

	  Choice  "Segment B000"
            pos[0]=XXXXXX0Xb
            pos[1]=10110XXXb
	    mem 0b0000h-0b3fffh

	  Choice  "Segment B400"
            pos[0]=XXXXXX1Xb
            pos[1]=10110XXXb
	    mem 0b4000h-0b7fffh

	  Choice  "Segment B800"
            pos[0]=XXXXXX0Xb
            pos[1]=10111XXXb
	    mem 0b8000h-0bbfffh

	  Choice  "Segment BC00"
            pos[0]=XXXXXX1Xb
            pos[1]=10111XXXb
	    mem 0bc000h-0bffffh

	  Choice  "Segment C000"
            pos[0]=XXXXXX0Xb
            pos[1]=11000XXXb
	    mem 0c0000h-0c3fffh

	Help
	"This selects the Address the AIP card will reside at.
	 Under normal circumstances, select <C400>."

nameditem
	Prompt	"Memory Chip Size"
	  Choice  "1 MByte SIMMS"
	    pos[0]=X0XXXXXXb
	  Choice  "4 MByte SIMMS"
	    pos[0]=X1XXXXXXb
	Help
	"This selects the size of the memory SIMMS installed in the AIP card.
	 Under normal circumstances, select <1 MByte SIMMS>."

nameditem
	Prompt	"AIP Card Option"
	  Choice  "Option 0"
	    pos[0]=XX0000XXb

	  Choice  "Option 1"
	    pos[0]=XX0001XXb

	  Choice  "Option 2"
	    pos[0]=XX0010XXb

	  Choice  "Option 3"
	    pos[0]=XX0011XXb

	  Choice  "Option 4"
	    pos[0]=XX0100XXb

	  Choice  "Option 5"
	    pos[0]=XX0101XXb

	  Choice  "Option 6"
	    pos[0]=XX0110XXb

	  Choice  "Option 7"
	    pos[0]=XX0111XXb

	  Choice  "Option 8"
	    pos[0]=XX1000XXb

	  Choice  "Option 9"
	    pos[0]=XX1001XXb

	  Choice  "Option 10"
	    pos[0]=XX1010XXb

	  Choice  "Option 11"
	    pos[0]=XX1011XXb

	  Choice  "Option 12"
	    pos[0]=XX1100XXb

	  Choice  "Option 13"
	    pos[0]=XX1101XXb

	  Choice  "Option 14"
	    pos[0]=XX1110XXb

	  Choice  "Option 15"
	    pos[0]=XX1111XXb

        Help
        "AIP card option.  Refer to the AIP card installation instructions
         for the appropriate setting."

nameditem
	Prompt	"Daughtercard Board Subtype"
	  Choice  "Subtype 0"
	    pos[0]=1XXXXXXXb
     pos[3]=XXXX1XXXb

	  Choice  "Subtype 1"
	    pos[0]=0XXXXXXXb
     pos[3]=XXXX1XXXb

	  Choice  "Subtype 2"
	    pos[0]=1XXXXXXXb
     pos[3]=XXXX0XXXb

	  Choice  "Subtype 3"
	    pos[0]=0XXXXXXXb
            pos[3]=XXXX0XXXb
        Help
        "Daughtercard board Subtype modifier.  If no daughtercard is installed
         on the AIP card, select <Subtype 0>.  If a daughtercard is installed
         see the hardware installation documention for the appropriate setting."

nameditem
	Prompt	"Daughtercard Option 0"
          Choice  "Off"
            pos[3]=XXXXXXX1b

          Choice  "On"
            pos[3]=XXXXXXX0b

        Help
        "Daughtercard option selector.  If no daughtercard is installed,
         select <Off>.  If a daughtercard is installed, refer to
         the hardware installation documentation for the appropriate setting."

nameditem
	Prompt	"Daughtercard Option 1"
          Choice  "Off"
            pos[3]=XXXXXX1Xb

          Choice  "On"
            pos[3]=XXXXXX0Xb

        Help
        "Daughtercard option selector.  If no daughtercard is installed,
         select <Off>.  If a daughtercard is installed, refer to
         the hardware installation documentation for the appropriate setting."

nameditem
	Prompt	"Daughtercard Option 2"
          Choice  "Off"
            pos[3]=XXXXX1XXb

          Choice  "On"
            pos[3]=XXXXX0XXb

        Help
        "Daughtercard option selector.  If no daughtercard is installed,
         select <Off>.  If a daughtercard is installed, refer to
         the hardware installation documentation for the appropriate setting."
