
AdapterId 0E04Fh

AdapterName  "3119 Adapter/A"

NumBytes 1

NamedItem

        Prompt "Adapter Memory Location"

        choice "Segment C000"

                pos[0] = 1111XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0C0000h - 0C1FFFh

        choice "Segment C200"

                pos[0] = 1110XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0C2000h - 0C3FFFh

        choice "Segment C400"

                pos[0] = 1101XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0C4000h - 0C5FFFh

        choice "Segment C600"

                pos[0] = 1100XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0C6000h - 0C7FFFh

        choice "Segment C800"

                pos[0] = 1011XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0C8000h - 0C9FFFh

        choice "Segment CA00"

                pos[0] = 1010XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0CA000h - 0CBFFFh

        choice "Segment CC00"

                pos[0] = 1001XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0CC000h - 0CDFFFh

        choice "Segment CE00"

                pos[0] = 1000XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0CE000h - 0CFFFFh

        choice "Segment D000"

                pos[0] = 0111XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0D0000h - 0D1FFFh

        choice "Segment D200"

                pos[0] = 0110XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0D2000h - 0D3FFFh

        choice "Segment D400"

                pos[0] = 0101XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0D4000h - 0D5FFFh

        choice "Segment D600"

                pos[0] = 0100XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0D6000h - 0D7FFFh

        choice "Segment D800"

                pos[0] = 0011XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0D8000h - 0D9FFFh

        choice "Segment DA00"

                pos[0] = 0010XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0DA000h - 0DBFFFh

        choice "Segment DC00"

                pos[0] = 0001XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0DC000h - 0DDFFFh

        choice "Segment DE00"

                pos[0] = 0000XXXXb
                io 0D78h - 0D7Fh
                int 7
                mem 0DE000h - 0DFFFFh



  Help

"To configure this adapter you must choose the memory
location the adapter will use to store data.
There are sixteen memory locations that can be selected.
Use the F5=Previous and the F6=Next keys to change this
assignment. Conflicting assignments are marked with
an asterisk and must be changed."

