AdapterId 0612Dh
AdapterName "DaynaTALK MC Network Adapter"
NumBytes 4

FixedResources	pos[3]=xxxx1010b

NamedItem

Prompt "Interrupt Level"

Choice "Level_5"   pos[0] = xxxx110xb   int 5
Choice "Level_4"   pos[0] = xxxx101xb   int 4
Choice "Level_3"   pos[0] = xxxx100xb   int 3
Choice "Polled"    pos[0] = xxxx111xb

Help
"Use the F5 = Previous and the F6 = Next keys to change the interrupt
level assignment.  If no free interrupt levels are available, use Polled, 
which is only slightly slower."



NamedItem

Prompt "I/O Address"

Choice "240-24F"   pos[1]=01000000b   pos[2]=00000010b   io 0240h-024Fh
Choice "260-26F"   pos[1]=01100000b   pos[2]=00000010b   io 0260h-026Fh
Choice "2A0-2aF"   pos[1]=10100000b   pos[2]=00000010b   io 02A0h-02AFh
Choice "320-32F"   pos[1]=00100000b   pos[2]=00000011b   io 0320h-032Fh
Choice "340-34F"   pos[1]=01000000b   pos[2]=00000011b   io 0340h-034Fh
Choice "200-20F"   pos[1]=00000000b   pos[2]=00000010b   io 0200h-020Fh

Help	
"A conflicting I/O address assignment is marked with an asterisk and must be
changed.  Use the F5 = Previous and the F6 = Next keys to change this 
assignment."

