
AdapterId 07FF9h

AdapterName "IOMEGA PC4 Host Adapter Board"

NumBytes 4


NamedItem
        Prompt  "Type of first fixed disk."
        Choice "32" pos[0]=XXXXXXXXb
        Choice "33" pos[0]=XXXXXXXXb 
        Choice "34" pos[0]=XXXXXXXXb 
        Choice "35" pos[0]=XXXXXXXXb 
        Choice "36" pos[0]=XXXXXXXXb 
        Choice "37" pos[0]=XXXXXXXXb 
        Choice "38" pos[0]=XXXXXXXXb 
        Choice "39" pos[0]=XXXXXXXXb 
        Choice "40" pos[0]=XXXXXXXXb 
        Choice "41" pos[0]=XXXXXXXXb 
        Choice "42" pos[0]=XXXXXXXXb 
        Choice "43" pos[0]=XXXXXXXXb 
        Choice "44" pos[0]=XXXXXXXXb 
        Choice "45" pos[0]=XXXXXXXXb 
        Choice "46" pos[0]=XXXXXXXXb 
        Choice "47" pos[0]=XXXXXXXXb 
        Choice "48" pos[0]=XXXXXXXXb 
 
 Help
"Select a drive type that matches the installed hard disk. 0 Indicates
no hard disk is installed. Valid drive types are 1 through 32."

NamedItem
        Prompt  "Type of second fixed disk."
        Choice "00" pos[0]=XXXXXXXXb
        Choice "33" pos[0]=XXXXXXXXb 
        Choice "34" pos[0]=XXXXXXXXb 
        Choice "35" pos[0]=XXXXXXXXb 
        Choice "36" pos[0]=XXXXXXXXb 
        Choice "37" pos[0]=XXXXXXXXb 
        Choice "38" pos[0]=XXXXXXXXb 
        Choice "39" pos[0]=XXXXXXXXb 
        Choice "40" pos[0]=XXXXXXXXb 
        Choice "41" pos[0]=XXXXXXXXb 
        Choice "42" pos[0]=XXXXXXXXb 
        Choice "43" pos[0]=XXXXXXXXb 
        Choice "44" pos[0]=XXXXXXXXb 
        Choice "45" pos[0]=XXXXXXXXb 
        Choice "46" pos[0]=XXXXXXXXb 
        Choice "47" pos[0]=XXXXXXXXb 
        Choice "48" pos[0]=XXXXXXXXb 

  Help
"Select a drive type that matches the installed hard disk. 0 Indicates
no hard disk is installed. Valid drive types are 1 through 32."


NamedItem
  Prompt "Host Adapter Board Interrupt Level"
      choice "INT LEVEL 5"     pos[0]=XX01XXXXb   INT 5
      choice "INT LEVEL 6"     pos[0]=XX00XXXXb   INT 6
      choice "INT LEVEL 7"     pos[0]=XX10XXXXb   INT 7
      choice "INT LEVEL 9"     pos[0]=XX11XXXXb   INT 9
    
  Help
"Set the Host Adapter Board Interrupt Level so it will not conflict with 
other interrupting devices.  Diskettes are usually level 6."



NamedItem
      Prompt "I/O Address Select"
      choice "240"        pos[0]=XXXX001Xb   io 00240h-0025Fh
      choice "340"   	  pos[0]=XXXX010Xb   io 00340h-0035Fh
      choice "400"        pos[0]=XXXX011Xb   io 00400h-0041Fh
      choice "420"        pos[0]=XXXX100Xb   io 00420h-0043Fh
      choice "3240"       pos[0]=XXXX101Xb   io 03240h-0325Fh
      choice "8240"       pos[0]=XXXX110Xb   io 08240h-0825Fh
      choice "A240"       pos[0]=XXXX111Xb   io 0A240h-0A25Fh
      choice "Disabled"	  pos[0]=XXXX000Xb

Help
"You may set the PC4 adapter to any one of the I/O Addresses
listed.  The first choice is recommended.  Make your selection
by using the F5=Previous or the F6=Next keys.  If your selection
conflicts with an I/O address already assigned in your system,
it will be marked with an asterisk and you must select an
alternate address."


NamedItem
      Prompt "DMA Level Select"
      choice "DMA Level 5"    pos[1]=1XXX0101b   arb 5
      choice "DMA Level 6"    pos[1]=1XXX0110b   arb 6
      choice "DMA Level 7"    pos[1]=1XXX0111b   arb 7

  Help
"The PC4 supports the direct memory access (DMA) mode of data
transfer.  Each DMA level has a corresponding priority level;
the lower the DMA level, the higher the corresponding priority.
You may select any one of the DMA levels listed by using the
F5=Previous or the F6=Next keys.  We recommend you select the
first level listed, DMA level 5.  If your selection conflicts
with a DMA level already assigned in the system, it will be
marked with an asterisk and you must select an alternative level."


NamedItem
      Prompt "Fairness"
      choice "Fairness Enabled"    pos[1]=XXX1XXXXb
      choice "Fairness Disabled"   pos[1]=XXX0XXXXb

  Help
"If 'Fairness' is enabled, the PC4 adapter will not compete for
the channel during the next arbitration phase if it is currently
in control of the channel.  This allows other installed adapters
to obtain the channel in the next sequence based on each adapter's
assigned priority level.  When 'Fairness' is disabled, the adapter
will compete for every arbitration phase and will obtain more than
its fair share of channel usage.  We recommend you use 'Fairness 
Enabled' for all adapters.  Select this option using the F5=Previous
and the F6=Next keys."


NamedItem
  Prompt "Preempt Count Select"
      choice "7 Bytes"    pos[1]=X11XXXXXb

  Help
"When the PC4 detects that another adapter requires use of the
channel, the Preempt Count feature is activated.  The Preempt
Count is the maximum number of bytes to transfer before yielding
control of the channel.  The PC4 will always transfer a maximum
of 7 bytes before relinquishing control of the channel."


NamedItem
  Prompt "Extended Data Area Select"
      choice "Data Select 0"       pos[2]=0000XXXXb   
   00.ADF

; If the configuration file does NOT have the NOWAITF1 flag then this file
; will be parsed in and displayed.

; Let SETUP know this will require a valid CMOS signature to have effect
PSignature

;******************************************************************
; CMOS 701 - POST F1 key control
;   bit 0 = Diskette error.
;           1 - Do not wait for F1 key
;           0 - Wait for F1 key
;   bit 1 = CRT (video) error.
;           1 - Do not wait for F1 key
;           0 - Wait fonded bios data
 area also.  The default is 80H, with increments of 80H."


