;Irwin 4100MC Configuration Diskette Program
;Irwin part no. 2908174
;File @707E.ADF
;Version 1.0
;Copyright (c) 1989 Cipher Data Products, Inc.
;All rights reserved.

AdapterId 707Eh

AdapterName "Irwin 4100MC Controller"

Numbytes 4

NamedItem

        Prompt  "I/O Addresses"
          choice "10F0h-10F7h" pos[1]=01000XXXb io 10f0h-10f7h
          choice "12F0h-12F7h" pos[1]=01001XXXb io 12f0h-12f7h
          choice "14F0h-14F7h" pos[1]=01010XXXb io 14f0h-14f7h
          choice "18F0h-18F7h" pos[1]=01100XXXb io 18f0h-18f7h
          choice "20F0h-20F7h" pos[1]=10000XXXb io 20f0h-20f7h
          choice "28F0h-28F7h" pos[1]=10100XXXb io 28f0h-28f7h
          choice "30F0h-30F7h" pos[1]=11000XXXb io 30f0h-30f7h

        Help
        "To configure this adapter you must choose the I/O addresses the adapter
         will use.  Use the F5=Previous and the F6=Next keys to change this
         assignment.  Conflicting assignments are marked with an asterisk and
         must be changed.  Under normal circumstances, select <10F0h-10F7h>."

NamedItem

        Prompt  "Interrupt Request Level"
          choice "5                       " pos[0]=01XXXXXXb int 5
          choice "6 (share with Diskette) " pos[0]=10XXXXXXb
          choice "10                      " pos[0]=00XXXXXXb int 10
          choice "11                      " pos[0]=11XXXXXXb int 11

        Help
         "This selects the interrupt level the adapter will use. This
          assignment need only be changed if it is in conflict with another
          assignment. Conflicting assignments are marked with an asterisk.  Use
          the F5=Previous and F6=Next keys to change interupt request level
          assignments.  Under normal circumstances, select <5>."

NamedItem

        Prompt  "Arbitration Level"
          choice "1                         " pos[3]=XXXX0001b arb 1
          choice "2 (share with Diskette)   " pos[3]=XXXX0010b
          choice "3                         " pos[3]=XXXX0011b arb 3
          choice "4                         " pos[3]=XXXX0100b arb 4
          choice "5                         " pos[3]=XXXX0101b arb 5
          choice "6                         " pos[3]=XXXX0110b arb 6
          choice "7                         " pos[3]=XXXX0111b arb 7

        Help
        "This selects the DMA channel the adapter will use to transfer data.
         This assignment need only be changed if it is in conflict with another
         assignment.  Conflicting assignments are marked with an asterisk.  Use
         the F5=Previous and the F6=Next keys to change arbitration level
         assigments.  Under normal circumstances, select <1>."

NamedItem

        Prompt  "Fairness On/Off"
          choice "On " pos[3]=XX10XXXXb
          choice "Off" pos[3]=XX11XXXXb

        Help
        "Fairness controls whether the adapter will release control of the bus
         to another device when it has been using it exclusively. Under normal
         circumstances, select <On>."
