
AdapterId 0E04Eh

AdapterName  "High Speed Adapter/A"

NumBytes 2

NamedItem

        Prompt "Adapter Memory Location"

        choice "Segment C800"

                pos[0] = 1011XXXXb
                io 0220h - 0227h
                int 7
                mem 0C8000h - 0C9FFFh

        choice "Segment CA00"

                pos[0] = 1010XXXXb
                io 0220h - 0227h
                int 7
                mem 0CA000h - 0CBFFFh

        choice "Segment CC00"

                pos[0] = 1001XXXXb
                io 0220h - 0227h
                int 7
                mem 0CC000h - 0CDFFFh

        choice "Segment CE00"

                pos[0] = 1000XXXXb
                io 0220h - 0227h
                int 7
                mem 0CE000h - 0CFFFFh

        choice "Segment D000"

                pos[0] = 0111XXXXb
                io 0220h - 0227h
                int 7
                mem 0D0000h - 0D1FFFh

        choice "Segment D200"

                pos[0] = 0110XXXXb
                io 0220h - 0227h
                int 7
                mem 0D2000h - 0D3FFFh

        choice "Segment D400"

                pos[0] = 0101XXXXb
                io 0220h - 0227h
                int 7
                mem 0D4000h - 0D5FFFh

        choice "Segment D600"

                pos[0] = 0100XXXXb
                io 0220h - 0227h
                int 7
                mem 0D6000h - 0D7FFFh

        choice "Segment D800"

                pos[0] = 0011XXXXb
                io 0220h - 0227h
                int 7
                mem 0D8000h - 0D9FFFh

        choice "Segment DA00"

                pos[0] = 0010XXXXb
                io 0220h - 0227h
                int 7
                mem 0DA000h - 0DBFFFh

        choice "Segment DC00"

                pos[0] = 0001XXXXb
                io 0220h - 0227h
                int 7
                mem 0DC000h - 0DDFFFh

        choice "Segment DE00"

                pos[0] = 0000XXXXb
                io 0220h - 0227h
                int 7
                mem 0DE000h - 0DFFFFh

  Help

"To configure this adapter you must choose the memory
location the adapter will use to store data.
There are twelve memory locations that can be selected.
Use the F5=Previous and the F6=Next keys to change this
assignment. Conflicting assignments are marked with
an asterisk and must be changed."

NamedItem

        Prompt "Channel B"

        choice "Full Duplex"    pos[0] = XXXXX1XXb

        choice "Half Duplex"    pos[0] = XXXXX0XXb

  Help
"This assignment is needed when you use Channel B.
This port can be assigned to function in either a
'Half Duplex' or 'Full Duplex' communication mode.
Use the F5=Previous and the F6=Next keys to change
this assignment."

