
AdapterId 06E79h

AdapterName "IRMA 3 3270 Coax Adapter"

NumBytes 4 

NamedItem
        Prompt "IRMA 3 Adapter Address"
      choice "200h-20Fh"  pos[0]=0000000xb io 0200h-020Fh
      choice "600h-60Fh"  pos[0]=0000001xb io 0600h-060Fh
      choice "A00h-A0Fh"  pos[0]=0000010xb io 0A00h-0A0Fh
      choice "E00h-E0Fh"  pos[0]=0000011xb io 0E00h-0E0Fh
      choice "240h-24Fh"  pos[0]=0001000xb io 0240h-024Fh
      choice "640h-64Fh"  pos[0]=0001001xb io 0640h-064Fh
      choice "A40h-A4Fh"  pos[0]=0001010xb io 0A40h-0A4Fh
      choice "E40h-E4Fh"  pos[0]=0001011xb io 0E40h-0E4Fh
      choice "260h-26Fh"  pos[0]=0001100xb io 0260h-026Fh
      choice "660h-66Fh"  pos[0]=0001101xb io 0660h-066Fh
      choice "A60h-A6Fh"  pos[0]=0001110xb io 0A60h-0A6Fh
      choice "E60h-E6Fh"  pos[0]=0001111xb io 0E60h-0E6Fh
      choice "2E0h-2EFh"  pos[0]=0011100xb io 02E0h-02EFh
      choice "6E0h-6EFh"  pos[0]=0011101xb io 06E0h-06EFh
      choice "AE0h-AEFh"  pos[0]=0011110xb io 0AE0h-0AEFh
      choice "EE0h-EEFh"  pos[0]=0011111xb io 0EE0h-0EEFh

   Help
     "This is the IRMA 3 adapter address. Sixteen choices
      are available :
                      200h - 20Fh
                      240h - 24Fh
                      260h - 26Fh
                      2E0h - 2EFh
                      600h - 60Fh
                      640h - 64Fh
                      660h - 66Fh
                      6E0h - 6EFh
                      A00h - A0Fh
                      A40h - A4Fh
                      A60h - A6Fh
                      AE0h - AEFh
                      E00h - E0Fh
                      E40h - E4Fh
                      E60h - E6Fh
                      EE0h - EEFh"

NamedItem
        Prompt "IRMA Emulator Port Address"
          Choice  "Enable 220-227"  
        pos[0] = xxxxxxxxb pos[1]=1xxxxxxxb io 0220h-0227h
          Choice  "Disable 220-227"  
        pos[0]=xxxxxxxxb pos[1] = 0xxxxxxxb  

   Help

          "The IRMA Emulator port Address is fixed at 220h. If the IRMA 
      Emulator Port address conflicts with another adapter board in the PC 
      you can: 
      1. Change the port address setting on the other board to resolve the 
         conflict or 
      2. Choose 'Disable 220 - 227'. Older DCA emulation software, such as 
         E78, and applications written for the original PROM board IRMA 
         product only run at address 220 - 227. If your software requires 
         this address 'Enable 220 - 227' must be selected. Current DCA 
         emulators, i.e. E78 PLUS, Irmax - Multisession and Irmax - DFT, can 
         be configured to use the four DCA emulator addresses selected below."

NamedItem
        Prompt "IRQ levels and disable interrupt"
      choice "IRQ2 "   pos[1]=xxx11000b int 2
      choice "IRQ10"   pos[1]=xxx11001b int 10
      choice "Disable INT"  pos[1]=xxx0xxxxb

   Help

      "When using IBM emulation software or DCA Irmax - DFT or 
      Irmax - Multisessions, IRQ2 (same as IRQ9) must be selected."

NamedItem
        Prompt "DCA Emulator Address"

      choice "280h-29Fh"
      pos[0]=xxxxx00xb pos[1]=x1xxxxxxb pos[2]=100xxxx0b io 0280h-029Fh
      choice "680h-69Fh"
      pos[0]=xxxxx01xb pos[1]=x1xxxxxxb pos[2]=100xxxx0b io 0680h-069Fh
      choice "A80h-A9Fh"
      pos[0]=xxxxx10xb pos[1]=x1xxxxxxb pos[2]=100xxxx0b io 0A80h-0A9Fh
      choice "E80h-E9Fh"
      pos[0]=xxxxx11xb pos[1]=x1xxxxxxb pos[2]=100xxxx0b io 0E80h-0E9Fh
      choice "2A0h-2BFh"
      pos[0]=xxxxx00xb pos[1]=x1xxxxxxb pos[2]=101xxxx0b io 02A0h-02BFh
      choice "6A0h-6BFh"
      pos[0]=xxxxx01xb pos[1]=x1xxxxxxb pos[2]=101xxxx0b io 06A0h-06BFh
      choice "AA0h-ABFh"
      pos[0]=xxxxx10xb pos[1]=x1xxxxxxb pos[2]=101xxxx0b io 0AA0h-0ABFh
      choice "EA0h-EBFh"
      pos[0]=xxxxx11xb pos[1]=x1xxxxxxb pos[2]=101xxxx0b io 0EA0h-0EBFh
      choice "2C0h-2DFh"
      pos[0]=xxxxx00xb pos[1]=x1xxxxxxb pos[2]=110xxxx0b io 02C0h-02DFh
      choice "6C0h-6DFh"
      pos[0]=xxxxx01xb pos[1]=x1xxxxxxb pos[2]=110xxxx0b io 06C0h-06DFh
      choice "AC0h-ADFh"
      pos[0]=xxxxx10xb pos[1]=x1xxxxxxb pos[2]=110xxxx0b io 0AC0h-0ADFh
      choice "EC0h-EDFh"
      pos[0]=xxxxx11xb pos[1]=x1xxxxxxb pos[2]=110xxxx0b io 0EC0h-0EDFh
      choice "220h-23Fh"
      pos[0]=xxxxx00xb pos[1]=01xxxxxxb pos[2]=001xxxx0b io 0220h-023Fh
      choice "620h-63Fh"
      pos[0]=xxxxx01xb pos[1]=x1xxxxxxb pos[2]=001xxxx0b io 0620h-063Fh
      choice "A20h-A3Fh"
      pos[0]=xxxxx10xb pos[1]=x1xxxxxxb pos[2]=001xxxx0b io 0A20h-0A3Fh
      choice "E20h-E3Fh"
      pos[0]=xxxxx11xb pos[1]=x1xxxxxxb pos[2]=001xxxx0b io 0E20h-0E3Fh
      choice  "Disable DCA" pos[1]=x0xxxxxxb  

   Help

      "Choose 2XX range If IRMA 3 ADAPTER ADDRESS setting is configured
      at 2XX range.  
      Choose 6XX range If IRMA 3 ADAPTER ADDRESS setting is configured
      at 6XX range.  
      Choose AXX range If IRMA 3 ADAPTER ADDRESS setting is configured
      at AXX range.  
      Choose EXX range If IRMA 3 ADAPTER ADDRESS setting is configured
      at EXX range.  
      Do not choose '220h - 23Fh' if 'IRMA Emulator Port Address'
      is at 'ENABLE 220-227'. 
      If the DCA Emulator Address conflicts with another adapter board
      in the PC you can :
      1. Change the port address setting on the other board to resolve 
         the conflict or 
      2. Choose one of the twelve alternate addresses and reconfigure
         IRMA 3 ADAPTER ADDRESS or
      3. Choose 'Disable DCA'"

NamedItem
        Prompt "IBM Emulator Port Address"
          choice "2D0h-2DFh"
          pos[0]=xxxxx00xb pos[1]=xx111000b pos[2]=xxxxxx01b io 02D0h - 02DFh int 2
          choice "6D0h-6DFh"
          pos[0]=xxxxx01xb pos[1]=xx111000b pos[2]=xxxxxx01b io 06D0h - 06DFh int 2
          choice "AD0h-ADFh"
          pos[0]=xxxxx10xb pos[1]=xx111000b pos[2]=xxxxxx01b io 0AD0h - 0ADFh int 2
          choice "ED0h-EDFh"
          pos[0]=xxxxx11xb pos[1]=xx111000b pos[2]=xxxxxx01b io 0ED0h - 0EDFh int 2

          choice "Disable IBM"
          pos[0]=xxxxxxxxb pos[2]=xxxxxxx0b

   Help

      "Choose 02D0h - 02DFH If IRMA 3 ADAPTER ADDRESS setting is configured
      at 2XX range.  
      Choose 06D0h - 06DFH If IRMA 3 ADAPTER ADDRESS setting is configured
      at 6XX range.  
      Choose 0AD0h - 0ADFH If IRMA 3 ADAPTER ADDRESS setting is configured
      at AXX range.  
      Choose 0ED0h - 0EDFH If IRMA 3 ADAPTER ADDRESS setting is configured
      at EXX range.  
      If these resources conflict with another adapter board in the pc
      you can: 
      1. Change the resource requirements on the other board to resolve
         the conflict or
      2. Choose one of the four alternate addresses and reconfigure
         IRMA 3 ADAPTER ADDRESS or
      3. Choose 'Disable IBM'. You cannot run IBM emulation software
         on IRMA 3 if IBM is disabled."

NamedItem
        Prompt "RAM Address Range"
  choice "CE000 - CFFFF"
      pos[1]=xx1xxxxxb pos[3]=xx011100b MEM 0CE000h - 0CFFFFh
  choice "CA000 - CBFFF"
      pos[1]=xx1xxxxxb pos[3]=xx010100b MEM 0CA000h - 0CBFFFh
  choice "CC000 - CDFFF"
      pos[1]=xx1xxxxxb pos[3]=xx011000b MEM 0CC000h - 0CDFFFh
  choice "D0000 - D1FFF"
      pos[1]=xx1xxxxxb pos[3]=xx100000b MEM 0D0000h - 0D1FFFh
  choice "D2000 - D3FFF"
      pos[1]=xx1xxxxxb pos[3]=xx100100b MEM 0D2000h - 0D3FFFh
  choice "D4000 - D5FFF"
      pos[1]=xx1xxxxxb pos[3]=xx101000b MEM 0D4000h - 0D5FFFh
  choice "D6000 - D7FFF"
      pos[1]=xx1xxxxxb pos[3]=xx101100b MEM 0D6000h - 0D7FFFh
  choice "D8000 - D9FFF"
      pos[1]=xx1xxxxxb pos[3]=xx110000b MEM 0D8000h - 0D9FFFh
  choice "DA000 - DBFFF"
      pos[1]=xx1xxxxxb pos[3]=xx110100b MEM 0DA000h - 0DBFFFh
  choice "DC000 - DDFFF"
      pos[1]=xx1xxxxxb pos[3]=xx111000b MEM 0DC000h - 0DDFFFh
  choice "DE000 - DFFFF"
      pos[1]=xx1xxxxxb pos[3]=xx111100b MEM 0DE000h - 0DFFFFh
  choice "Disable RAM"
        pos[1]=xx0xxxxxb pos[3]=xx0000xxb

   Help

      "When using IBM emulation software Ram Address Range must
      be selected. If the Ram Address Range conflicts with another 
      adapter in the PC you can : 
      1. Change the ram address setting on the other board to
         resolve the conflict or  
      2. Choose one of the eleven memory addresses and configure
         the DCA emulator to use the new address or  
      3. Choose 'Disable Ram'. You cannot run IBM emulation
         software on IRMA 3 if disable ram is selected."
