
AdapterID 06ee7h

AdapterName  "IMC Networks Corporation  PCnic II Ethernet Controller"

NumBytes 2

nameditem
        Prompt  "Interrupt Level Select"
          Choice  "IRQ Level 3"
            pos[0]=XXXX110Xb
            int 3
          Choice  "IRQ Level 5"
            pos[0]=XXXX101Xb
            int 5
          Choice  "IRQ Level 10"
            pos[0]=XXXX100Xb
            int 10
          Choice  "IRQ Level 11"
            pos[0]=XXXX011Xb
            int 11
          Choice  "IRQ Level 15"
            pos[0]=XXXX010Xb
            int 15
        Help
        "This selects the interrupt level the adapter will use to request
	 service from the PS/2 computer. Under normal circumstances, 
	 select <Level 3>."

nameditem
        Prompt  "I/O Port Select"
		    Choice  "I/O Base F200"
			   pos[1]=00100000b
		 io 0F200h-0F207h
          Choice  "I/O Base F280"
            pos[1]=00101000b
	    io 0F280h-0F287h
          Choice  "I/O Base F2A0"
            pos[1]=00101010b
	    io 0F2A0h-0F2A7h
          Choice  "I/O Base F2C0"
            pos[1]=00101100b
	    io 0F2C0h-0F2C7h
          Choice  "I/O Base F2E0"
            pos[1]=00101110b
	    io 0F2E0h-0F2E7h
          Choice  "I/O Base F300"
            pos[1]=00110000b
	    io 0F380h-0F307h
          Choice  "I/O Base F320"
            pos[1]=00110010b
	    io 0F320h-0F327h
          Choice  "I/O Base F340"
            pos[1]=00110100b
	    io 0F340h-0F347h
          Choice  "I/O Base F360"
            pos[1]=00110110b
	    io 0F360h-0F367h
          Choice  "I/O Base F380"
	         pos[1]=00111000b
	    io 0F380h-0F387h
	Help
	"This selects the I/O address range to which the adapter will respond
	 when addressed by the PS/2 computer. Eight contiguous addresses
	 are used by the adapter. More ranges can be defined if these conflict."



					  

