; 
;	$Revision:   1.3  $
;	$Date:   09 Dec 1991 15:09:22  $
; 
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  			   *
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterID 0eeffh

ADAPTERNAME  "IBM Dual Async Adapter"

NUMBYTES 1

NAMEDITEM
	PROMPT  "Connector 1"
	CHOICE  "SERIAL_1"   pos[0]=XXXX000Xb  int 4   io 03f8h-03ffh   
	CHOICE  "SERIAL_2"   pos[0]=XXXX001Xb  int 3   io 02f8h-02ffh   
	CHOICE  "SERIAL_3"   pos[0]=XXXX010Xb  int 3   io 3220h-3227h
	CHOICE  "SERIAL_4"   pos[0]=XXXX011Xb  int 3   io 3228h-0322fh
	CHOICE  "SERIAL_5"   pos[0]=XXXX100Xb  int 3   io 4220h-4227h 
	CHOICE  "SERIAL_6"   pos[0]=XXXX101Xb  int 3   io 4228h-0422fh
	CHOICE  "SERIAL_7"   pos[0]=XXXX110Xb  int 3   io 5220h-5227h 
	CHOICE  "SERIAL_8"   pos[0]=XXXX111Xb  int 3   io 5228h-0522fh
	HELP
	   "This connector on the IBM Dual Async Adapter can be 
assigned to use SERIAL_1 through SERIAL_8.  Use the F5=previous and 
the F6=Next keys to change serial port assignments if you are in the 
'Change Configuration' window.  Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."




NAMEDITEM
	PROMPT  "Connector 2"
	CHOICE  "SERIAL_1"   pos[0]=1000XXXXb   int 4   io 03f8h-03ffh   
	CHOICE  "SERIAL_2"   pos[0]=1001XXXXb   int 3   io 02f8h-02ffh   
	CHOICE  "SERIAL_3"   pos[0]=1010XXXXb	int 3   io 3220h-3227h
	CHOICE  "SERIAL_4"   pos[0]=1011XXXXb	int 3	io 3228h-0322fh
	CHOICE  "SERIAL_5"   pos[0]=1100XXXXb	int 3   io 4220h-4227h 
	CHOICE  "SERIAL_6"   pos[0]=1101XXXXb	int 3	io 4228h-0422fh
	CHOICE  "SERIAL_7"   pos[0]=1110XXXXb   int 3	io 5220h-5227h 
	CHOICE  "SERIAL_8"   pos[0]=1111XXXXb	int 3	io 5228h-0522fh
	HELP
	   "This connector on the IBM Dual Async Adapter can be 
assigned to use SERIAL_1 through SERIAL_8.  Use the F5=previous and 
the F6=Next keys to change serial port assignments if you are in the 
'Change Configuration' window.  Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."
