; Adapter Description File for the ActionMedia (TM) Series II Board on
; the Microchannel Architecture
; Copyright 1990,1991 Intel Corporation.
; All Rights Reserved.

AdapterID 0EFDCh

AdapterName "Intel DS2 Adapter -- 12 July 1991"

NumBytes 4

NamedItem Prompt "Enable/Disable Adapter"
  Choice "Enable"    POS[0]=XXXXXXX1b
  Choice "Disable"   POS[0]=XXXXXXX0b
  Help
"ENABLE/DISABLE ADAPTER:  This controls whether the adapter is enabled or not.
Use the ENABLED setting for normal use.  Use the DISABLED setting if you are
not using the adapter and enabling it causes a conflict with another device."


NamedItem Prompt "I/O Address Range"
  Choice "C000 - C03F"   POS[1]=110000XXb   IO 0C000h - 0C03Fh
  Choice "C400 - C43F"   POS[1]=110001XXb   IO 0C400h - 0C5FFh
  Choice "C800 - C83F"   POS[1]=110010XXb   IO 0C800h - 0C9FFh
  Choice "CC00 - CC3F"   POS[1]=110011XXb   IO 0CC00h - 0CDFFh
  Choice "B000 - B03F"   POS[1]=101100XXb   IO 0B000h - 0B1FFh
  Choice "B400 - B43F"   POS[1]=101101XXb   IO 0B400h - 0B5FFh
  Choice "B800 - B83F"   POS[1]=101110XXb   IO 0B800h - 0B9FFh
  Choice "BC00 - BC3F"   POS[1]=101111XXb   IO 0BC00h - 0BDFFh
  Help
"I/O ADDRESS RANGE:  This adapter occupies 64 bytes of I/O space.
This may be located on any of the available 1024 byte boundaries.
Use 'C000 - C03F' unless there is a conflict."


NamedItem Prompt "VRAM Window Size and Starting Address"

  Choice " 8K - C0000"   POS[3]=10000110b   POS[2]=0000XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0C0000h - 0C1FFFh
  Choice " 8K - C2000"   POS[3]=10000110b   POS[2]=0001XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0C2000h - 0C3FFFh
  Choice " 8K - C4000"   POS[3]=10000110b   POS[2]=0010XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0C4000h - 0C5FFFh
  Choice " 8K - C6000"   POS[3]=10000110b   POS[2]=0011XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0C6000h - 0C7FFFh
  Choice " 8K - C8000"   POS[3]=10000110b   POS[2]=0100XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0C8000h - 0C9FFFh
  Choice " 8K - CA000"   POS[3]=10000110b   POS[2]=0101XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0CA000h - 0CBFFFh
  Choice " 8K - CC000"   POS[3]=10000110b   POS[2]=0110XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0CC000h - 0CDFFFh
  Choice " 8K - CE000"   POS[3]=10000110b   POS[2]=0111XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0CE000h - 0CFFFFh

  Choice " 8K - D0000"   POS[3]=10000110b   POS[2]=1000XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0D0000h - 0D1FFFh
  Choice " 8K - D2000"   POS[3]=10000110b   POS[2]=1001XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0D2000h - 0D3FFFh
  Choice " 8K - D4000"   POS[3]=10000110b   POS[2]=1010XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0D4000h - 0D5FFFh
  Choice " 8K - D6000"   POS[3]=10000110b   POS[2]=1011XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0D6000h - 0D7FFFh
  Choice " 8K - D8000"   POS[3]=10000110b   POS[2]=1100XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0D8000h - 0D9FFFh
  Choice " 8K - DA000"   POS[3]=10000110b   POS[2]=1101XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0DA000h - 0DBFFFh
  Choice " 8K - DC000"   POS[3]=10000110b   POS[2]=1110XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0DC000h - 0DDFFFh
  Choice " 8K - DE000"   POS[3]=10000110b   POS[2]=1111XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb   MEM 0DE000h - 0DFFFFh

  Choice "32K - C0000"   POS[3]=10000110b   POS[2]=0000XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb   MEM 0C0000h - 0C7FFFh
  Choice "32K - C8000"   POS[3]=10000110b   POS[2]=0100XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb   MEM 0C8000h - 0CFFFFh
  Choice "32K - D0000"   POS[3]=10000110b   POS[2]=1000XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb   MEM 0D0000h - 0D7FFFh
  Choice "32K - D8000"   POS[3]=10000110b   POS[2]=1100XXXXb   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb   MEM 0D8000h - 0DFFFFh

  Help
"VRAM WINDOW SIZE AND STARTING ADDRESS:  Select the combination of vram
window size and starting address.  AVK based software can use either 8K
or 32K windows while ActionMedia requires a 32K window."


NamedItem Prompt "Video Interrupt Level"
  Choice "Level  9"   POS[2]=XXXX00XXb   INT 9d
  Choice "Level 10"   POS[2]=XXXX01XXb   INT 10d
  Choice "Level 11"   POS[2]=XXXX10XXb   INT 11d
  Choice "Level 12"   POS[2]=XXXX11XXb   INT 12d
  Help
"VIDEO INTERRUPT LEVEL:  This adapter can use one of interrupt levels 9 - 12
for Video interrupts."


NamedItem Prompt "Audio Interrupt Level"
  Choice "Level 10"   POS[2]=XXXXXX0Xb   INT 10d
  Choice "Level 11"   POS[2]=XXXXXX1Xb   INT 11d
  Help
"AUDIO INTERRUPT LEVEL:  This adapter can use one of interrupt levels 10 or 11
for Audio interrupts."


NamedItem Prompt "CS2 EO Interrupt Level"
  Choice "Level 10"   POS[2]=XXXXXXX0b   INT 10d
  Choice "Level 11"   POS[2]=XXXXXXX1b   INT 11d
  Help
"CS2 EO INTERRUPT LEVEL:  This adapter can use one of interrupt levels 10 or 11
for CS2 Even/Odd interrupts."


NamedItem Prompt "Enable/Disable POST Program"
  Choice "Enable"    POS[1]=XXXXXXX1b
  Choice "Disable"   POS[1]=XXXXXXX0b
  Help
"ENABLE/DISABLE POST PROGRAM:  This controls whether the adapter's Power On
Self Test program is run at system initialization time.  Use the ENABLED
setting for normal use."


NamedItem Prompt "POST Prom Address Range"

  Choice "C0000 - C1FFF"   POS[0]=0000XXXXb   MEM 0C0000h - 0C1FFFh
  Choice "C2000 - C3FFF"   POS[0]=0001XXXXb   MEM 0C2000h - 0C3FFFh
  Choice "C4000 - C5FFF"   POS[0]=0010XXXXb   MEM 0C4000h - 0C5FFFh
  Choice "C6000 - C7FFF"   POS[0]=0011XXXXb   MEM 0C6000h - 0C7FFFh
  Choice "C8000 - C9FFF"   POS[0]=0100XXXXb   MEM 0C8000h - 0C9FFFh
  Choice "CA000 - CBFFF"   POS[0]=0101XXXXb   MEM 0CA000h - 0CBFFFh
  Choice "CC000 - CDFFF"   POS[0]=0110XXXXb   MEM 0CC000h - 0CDFFFh
  Choice "CE000 - CFFFF"   POS[0]=0111XXXXb   MEM 0CE000h - 0CFFFFh

  Choice "D0000 - D1FFF"   POS[0]=1000XXXXb   MEM 0D0000h - 0D1FFFh
  Choice "D2000 - D3FFF"   POS[0]=1001XXXXb   MEM 0D2000h - 0D3FFFh
  Choice "D4000 - D5FFF"   POS[0]=1010XXXXb   MEM 0D4000h - 0D5FFFh
  Choice "D6000 - D7FFF"   POS[0]=1011XXXXb   MEM 0D6000h - 0D7FFFh
  Choice "D8000 - D9FFF"   POS[0]=1100XXXXb   MEM 0D8000h - 0D9FFFh
  Choice "DA000 - DBFFF"   POS[0]=1101XXXXb   MEM 0DA000h - 0DBFFFh
  Choice "DC000 - DDFFF"   POS[0]=1110XXXXb   MEM 0DC000h - 0DDFFFh
  Choice "DE000 - DFFFF"   POS[0]=1111XXXXb   MEM 0DE000h - 0DFFFFh

  Help
"POST PROM ADDRESS RANGE: The adapter needs an 8K block of host address space
for use only when the POST program runs."
