
AdapterId 05125h

AdapterName "Micro Channel Tape Drive Host Adapter"   

NumBytes 2

NamedItem
Prompt "Host Adapter I/O Base Address"
choice " 338"    pos[0]=XXXX001Xb  io 0338h-0339h
choice " 368"    pos[0]=XXXX010Xb  io 0368h-0369h
choice " 398"    pos[0]=XXXX011Xb  io 0398h-0399h
choice " 200"    pos[0]=XXXX100Xb  io 0200h-0201h
choice " 238"    pos[0]=XXXX101Xb  io 0238h-0239h
choice " 310"    pos[0]=XXXX110Xb  io 0310h-0311h

Help
"Each device attached to the computer requires one or
more I/O addresses to communicate with the computer.   
Press the F5 (for previous) or F6 (for next) function key
to assign a different value to this port. An * (asterisk)
will appear beside the setting when it conflicts with 
another device on your system. You can scroll through the
configuration menu to locate other devices configured on
your system and the base addresses they use."

NamedItem
Prompt "Host Adapter Interrupt Number"
choice " 3"   pos[0]=XX00XXXXb  int  3
choice " 4"   pos[0]=XX01XXXXb  int  4
choice " 5"   pos[0]=XX10XXXXb  int  5
choice " 6"   pos[0]=XX11XXXXb  int  6

Help
"In order for a device to alert the computer that it is
ready to receive instructions, it signals the computer
by using interrupts. Press the F5 (for previous) or F6 
(for next) function key to assign a different value. 
You will not be informed when you select an interrupt
that is currently in use on your system. Consequently,
you should scroll through the configuration menu to 
locate other devices configured on your system and 
the interrupts in use."

NamedItem
Prompt "Host Adapter DMA Channel"
choice " 1"   pos[1]=XXXX0001b  arb  1
choice " 3"   pos[1]=XXXX0011b  arb  3
choice " 0"   pos[1]=XXXX0000b  arb  0

Help
"The Tape Drive Host Adapter uses a DMA channel to transfer 
data between disks and the tape drive. Press the F5 
(for previous) or F6 (for next) function key to assign 
a different value. An * (asterisk) will appear beside 
the setting when it conflicts with another device on 
your system. You can scroll through the configuration 
menu to locate other devices configured on your system
and the DMA channels in use."
