AdapterID 05023h

AdapterName  "PCM Audio Record/Playback Unit"

NumBytes 2

nameditem
	Prompt  "Adapter IO Location"
	   Choice "DSA_1"
	      pos[0]=000000xxb
	      io 0400h-040Fh
	   Choice "DSA_2"
	      pos[0]=000001xxb
	      io 0420h-042Fh
	   Choice "DSA_3"
	      pos[0]=000010xxb
	      io 0440h-044Fh
	   Choice "DSA_4"
	      pos[0]=000100xxb
	      io 0480h-048Fh
	   Choice "DSA_5"
	      pos[0]=001000xxb
	      io 0500h-050Fh
	   Choice "DSA_6"
	      pos[0]=010000xxb
	      io 4400h-440Fh
	   Choice "DSA_7"
	      pos[0]=100000xxb
	      io 8400h-840Fh
	   Choice "DSA_8"
	      pos[0]=111111xxb
	      io 0C5E0h-0C5EFh
	   Choice "DSA_9"
	      pos[0]=001001xxb
	      io 0520h-052Fh
	   Choice "DSA_10"
	      pos[0]=001010xxb
	      io 0540h-054Fh
	   Choice "DSA_11"
	      pos[0]=001111xxb
	      io 05E0h-05EFh
	   Choice "DSA_12"
	      pos[0]=110000xxb
	      io 0C400h-0C40Fh
	   Choice "DSA_13"
	      pos[0]=110011xxb
	      io 0C460h-0C46Fh
	   Choice "DSA_14"
	      pos[0]=111011xxb
	      io 0C560h-0C56Fh
	      
	Help
	"To configure this adapter, you must choose the IO loaction the
	adapter will use for its Base Address.  There are eight locations 
	supported.  Choose <DSA_1> unless there is a conflict."
	
nameditem
	Prompt "Interrupt Level"
           Choice "Interrupt Level 3"
	      pos[1]=xxxx0011b
	      int 3
	   Choice "Interrupt Level 4"
	      pos[1]=xxxx0100b
	      int 4
	   Choice "Interrupt Level 5"
	      pos[1]=xxxx0101b
	      int 6
	   Choice "Interrupt Level 6"
	      pos[1]=xxxx0110b
	      int 6
	   Choice "Interrupt Level 7"
	      pos[1]=xxxx0111b
	      int 6
	   Choice "Interrupt Level 9"
	      pos[1]=xxxx1001b
	      int 9
	   Choice "Interrupt Level 10"
	      pos[1]=xxxx1010b
	      int 10
	   Choice "Interrupt Level 11"
	      pos[1]=xxxx1011b
	      int 6
	   Choice "Interrupt Level 12"
	      pos[1]=xxxx1100b
	      int 6
	   Choice "Interrupt Level 14"
	      pos[1]=xxxx1110b
	      int 6
	   Choice "Interrupt Level 15"
	      pos[1]=xxxx1111b
	      int 15
	   Choice "Interrupts Disabled"
	      pos[1]=xxxx0000b
	      
	   Help
	   "This selects the interrupt level used to alert the system processor 
	   of status changes.  Normally, <Interrupt Level 4> should be selected."
	      
nameditem
	Prompt  "DMA Arbitration Level"
	   Choice "Arb_Level 7"
	      pos[1]=0111xxxxb
	      arb 7
	   Choice "Arb_Level 0"
	      pos[1]=0000xxxxb
	      arb 0
	   Choice "Arb_Level 1"
	      pos[1]=0001xxxxb
	      arb 1
	   Choice "Arb_Level 2"
	      pos[1]=0010xxxxb
	      arb 2
	   Choice "Arb_Level 3"
	      pos[1]=0011xxxxb
	      arb 3
	   Choice "Arb_Level 4"
	      pos[1]=0100xxxxb
	      arb 4
	   Choice "Arb_Level 5"
	      pos[1]=0101xxxxb
	      arb 5
	   Choice "Arb_Level 6"
	      pos[1]=0110xxxxb
	      arb 6
	      
	   Help
	   "This selects the DMA channel the adapter will use to transfer
	   data.  Normally, <Arb_Level 7> should be selected unless there 
           is a conflict."


