
AdapterId 07011h

AdapterName "Tecmar MicroRAM AD Multifunction Board"

NumBytes 6

FixedResources
	POS[0]=00000001b

NamedItem
        Prompt "EMS Board Select"
      choice "Board 1"    pos[2]=100XXXXXb  io 0270h-0277h
      choice "Board 2"    pos[2]=010XXXXXb  io 0370h-0377h
      choice "Board 3"    pos[2]=110XXXXXb  io 0670h-0677h
      choice "Board 4"    pos[2]=001XXXXXb  io 0770h-0777h
      choice "Board 5"    pos[2]=101XXXXXb  io 0A70h-0A77h
      choice "Board 6"    pos[2]=011XXXXXb  io 0B70h-0B77h
      choice "Board 7"    pos[2]=111XXXXXb  io 0E70h-0E77h
      choice "Disable"    pos[2]=000XXXXXb

   Help
 "The EMS page registers can be disabled or assigned to any of seven (7)
 I/O locations.  Use the F5=Previous and the F6=Next keys to change this
 assignment in the 'Change configuration' window.  Conflicting
 assignments are marked with an asterisk and must be changed to
 use the adapter."

NamedItem
        Prompt "Serial Port 1 Interrupt Select"
      choice "Int  3 "   pos[2]=XXXXXX00b  int  3
      choice "Int  4 "   pos[2]=XXXXXX01b  int  4
      choice "Int  5 "   pos[2]=XXXXXX10b  int  5
      choice "Int  9 "   pos[2]=XXXXXX11b  int  9

   Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."

NamedItem
        Prompt "Serial Port 1 Address Select"
      choice "Disable"   pos[3]=XXXXXX0Xb
      choice "COM1   "   pos[3]=XXX00X1Xb  io  03F8h-03FFh
      choice "COM2   "   pos[3]=XXX01X1Xb  io  02F8h-02FFh
      choice "COM3   "   pos[3]=XXX10X1Xb  io  03E8h-03EFh
      choice "COM4   "   pos[3]=XXX11X1Xb  io  02E8h-02EFh

  Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."

NamedItem
        Prompt "Serial Port 2 Interrupt Select"
      choice "Int  4 "   pos[2]=XXXX01XXb  int  4
      choice "Int  3 "   pos[2]=XXXX00XXb  int  3
      choice "Int  5 "   pos[2]=XXXX10XXb  int  5
      choice "Int  9 "   pos[2]=XXXX11XXb  int  9

   Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."

NamedItem
        Prompt "Serial Port 2 Address Select"
      choice "Disable"   pos[3]=1XXXX0XXb
      choice "COM2   "   pos[3]=100XX1XXb  io  02F8h-02FFh
      choice "COM3   "   pos[3]=101XX1XXb  io  03E8h-03EFh
      choice "COM4   "   pos[3]=110XX1XXb  io  02E8h-02EFh

  Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."




