; 
;	$Revision:   1.3  $
;	$Date:   09 Dec 1991 15:09:10  $
; 
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  			   *
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterID 0deffh

ADAPTERNAME  "IBM Multi-Protocol Communications Adapter"

NUMBYTES 2

NAMEDITEM 
	PROMPT	"Communications Port"
	CHOICE  "SDLC_1"   int 3 4   io 0380h-038fh    pos[0]=XXX1000Xb
	CHOICE  "SDLC_2"   int 3 4   io 03a0h-03afh    pos[0]=XXX1001Xb
	CHOICE  "BISYNC_1"   int 3 4  io 03a0h-03afh   pos[0]=XXX1100Xb
	CHOICE  "BISYNC_2"   int 3 4  io 0380h-038fh   pos[0]=XXX1101Xb
	CHOICE  "SERIAL_1"   int 4   io	03f8h-03ffh    pos[0]=XXX0000Xb
	CHOICE  "SERIAL_2"   int 3   io 02f8h-02ffh    pos[0]=XXX0001Xb
	CHOICE  "SERIAL_3"   int 3   io	3220h-3227h    pos[0]=XXX0010Xb
	CHOICE  "SERIAL_4"   int 3   io	3228h-0322fh   pos[0]=XXX0011Xb
	CHOICE  "SERIAL_5"   int 3   io	4220h-4227h    pos[0]=XXX0100Xb
	CHOICE  "SERIAL_6"   int 3   io 4228h-0422fh   pos[0]=XXX0101Xb
	CHOICE  "SERIAL_7"   int 3   io	5220h-5227h    pos[0]=XXX0110Xb
	CHOICE  "SERIAL_8"   int 3   io	5228h-0522fh   pos[0]=XXX0111Xb
	HELP
	   "This port can be assigned as a:  primary (SDLC_1) or 
secondary (SDLC_2) sdlc, primary (BISYNC_1) or secondary (BISYNC_2) 
bisync, or as serial port (SERIAL_1 through SERIAL_8).  Use the 
F5=Previous and the F6=Next keys to change this assignment in the 
'Change Configuration' window.  Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."


NAMEDITEM 
	PROMPT	"Arbitration Level for SDLC"
	CHOICE  "Level_1"   pos[1]=XXXX0001b   arb 1
	CHOICE  "Level_7"   pos[1]=XXXX0111b   arb 7
	CHOICE  "Level_0"   pos[1]=XXXX0000b   arb 0
	CHOICE  "Level_2"   pos[1]=XXXX0010b   arb 2
	CHOICE  "Level_3"   pos[1]=XXXX0011b   arb 3
	CHOICE  "Level_4"   pos[1]=XXXX0100b   arb 4
	CHOICE  "Level_5"   pos[1]=XXXX0101b   arb 5
	CHOICE  "Level_6"   pos[1]=XXXX0110b   arb 6
	CHOICE  "Level_8"   pos[1]=XXXX1000b   arb 8
	CHOICE  "Level_9"   pos[1]=XXXX1001b   arb 9
	CHOICE  "Level_10"   pos[1]=XXXX1010b   arb 10
	CHOICE  "Level_11"   pos[1]=XXXX1011b   arb 11
	CHOICE  "Level_12"   pos[1]=XXXX1100b   arb 12
	CHOICE  "Level_13"   pos[1]=XXXX1101b   arb 13
	CHOICE  "Level_14"   pos[1]=XXXX1110b   arb 14
	HELP
	   "This assignment need only be changed if it is in conflict 
with another assignment.  Conflicting assignments are marked with an 
asterisk.  Use the F5=Previous and the F6=Next keys to change 
arbitration level assignments if you are in the 'Change 
Configuration' window."



