
AdapterId 06203h

AdapterName  "QUADPORT PS/Q  I/O Adapter  R2 9087"

NumBytes 2

NamedItem
        Prompt "Serial Port  A "
      choice "SERIAL_1"  pos[0]=XXX110XXb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXX000XXb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXX001XXb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXX010XXb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXX011XXb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXX100XXb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXX101XXb  io 5220h-5227h  int 3
      choice "DISABLED"  pos[0]=XXX111XXb
   Help
"This connector on the QUADPORT PS/Q IO Adapter can be
assigned to use Serial 1 through Serial 7.  Use the
F5=Previous and the F6=Next keys to change serial port
assignments if you are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."

NamedItem
        Prompt "Serial Port  B "
      choice "SERIAL_1"  pos[0]=110XXXXXb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=000XXXXXb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=001XXXXXb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=010XXXXXb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=011XXXXXb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=100XXXXXb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=101XXXXXb  io 5220h-5227h  int 3
      choice "DISABLED"  pos[0]=111XXXXXb
   Help
"This connector on the QUADPORT PS/Q IO Adapter can be
assigned to use Serial 1 through Serial 7.  Use the
F5=Previous and the F6=Next keys to change serial port
assignments if you are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."

