
AdapterId 06784h

AdapterName  "NEOTECH DUAL RS-422/RS-485 SERIAL ADAPTER"

NumBytes 1

NamedItem
        Prompt "COMn"       
      choice "RS-422 COM2/COM3 IRQ3"  pos[0]=00010001b  io 02F8h-02FFh 
						           3220h-3227h int 3

      choice "RS-422 COM2/COM3 IRQ4"  pos[0]=00100001b  io 02F8h-02FFh 
							   3220h-3227h int 4
      choice "RS-422 COM2/COM3 IRQ7"  pos[0]=01000001b  io 02F8h-02FFh 
							   3220h-3227h int 7
      choice "RS-422 COM2/COM3 IRQ9"  pos[0]=10000001b  io 02F8h-02FFh 
							   3220h-3227h int 9

      choice "RS-422 COM3/COM4 IRQ3"  pos[0]=00010011b  io 3220h-322Fh int 3
      choice "RS-422 COM3/COM4 IRQ4"  pos[0]=00100011b  io 3220h-322Fh int 4
      choice "RS-422 COM3/COM4 IRQ7"  pos[0]=01000011b  io 3220h-322Fh int 7
      choice "RS-422 COM3/COM4 IRQ9"  pos[0]=10000011b  io 3220h-322Fh int 9


      choice "RS-422 COM4/COM5 IRQ3"  pos[0]=00010101b  io 3228h-322Fh 
							   4220h-4227h int 3
      choice "RS-422 COM4/COM5 IRQ4"  pos[0]=00100101b  io 3228h-322Fh 
							   4220h-4227h int 4
      choice "RS-422 COM4/COM5 IRQ7"  pos[0]=01000101b  io 3228h-322Fh 
							   4220h-4227h int 7
      choice "RS-422 COM4/COM5 IRQ9"  pos[0]=10000101b  io 3228h-322Fh 
							   4220h-4227h int 9


      choice "RS-485 COM2/COM3 IRQ3"  pos[0]=00011001b  io 02F8h-02FFh
							   3220h-3227h int 3
      choice "RS-485 COM2/COM3 IRQ4"  pos[0]=00101001b  io 02F8h-02FFh
							   3220h-3227h int 4
      choice "RS-485 COM2/COM3 IRQ7"  pos[0]=01001001b  io 02F8h-02FFh
							   3220h-3227h int 7
      choice "RS-485 COM2/COM3 IRQ9"  pos[0]=10001001b  io 02F8h-02FFh
							   3220h-3227h int 9


      choice "RS-485 COM3/COM4 IRQ3"  pos[0]=00011011b  io 3220h-322Fh int 3
      choice "RS-485 COM3/COM4 IRQ4"  pos[0]=00101011b  io 3220h-322Fh int 4
      choice "RS-485 COM3/COM4 IRQ7"  pos[0]=01001011b  io 3220h-322Fh int 7
      choice "RS-485 COM3/COM4 IRQ9"  pos[0]=10001011b  io 3220h-322Fh int 9

      choice "RS-485 COM4/COM5 IRQ3"  pos[0]=00011101b  io 3228h-322Fh
							   4220h-4227h int 3
      choice "RS-485 COM4/COM5 IRQ4"  pos[0]=00101101b  io 3228h-322Fh
							   4220h-4227h int 4
      choice "RS-485 COM4/COM5 IRQ7"  pos[0]=01001101b  io 3228h-322Fh
							   4220h-4227h int 7
      choice "RS-485 COM4/COM5 IRQ9"  pos[0]=10001101b  io 3228h-322Fh
							   4220h-4227h int 9



   Help
"This allows you to set the two serial channels to be 'COM2/COM3',
 COM3/COM4, COM4/COM5, or COM5/COM6. Use the F5=Previous and the 
 F6=Next keys to change serial port assignments if you are in the 
 'Change configuration' window. Conflicting assignments are marked 
 with an asterisk and must be changed to use the adapter."
	

