 
AdapterId 00EFFh
 
AdapterName "BNR PSDO Card"
 
NumBytes 2
 
NamedItem
 
       Prompt "Arbitration Level for PSDO card"
 
       Choice "Level_5" pos[0]=xxx0101xb       arb 5
       Choice "Level_6" pos[0]=xxx0110xb       arb 6
       Choice "Level_7" pos[0]=xxx0111xb       arb 7
       Choice "Level_3" pos[0]=xxx0011xb       arb 3
 
       Help
"Use the F5=Previous and F6=Next keys to
 change the arbitration level assignments.
 An arbitration level of 0 has the highest
 priority, and increasing levels have
 corresponding decreased priority."
 
 
NamedItem
 
       Prompt "Soft Interrupt for PSDO Driver"
 
        Choice "66h" pos[0]=110xxxxxb
        Choice "67h" pos[0]=111xxxxxb
        Choice "60h" pos[0]=000xxxxxb
        Choice "61h" pos[0]=001xxxxxb
        Choice "62h" pos[0]=010xxxxxb
        Choice "63h" pos[0]=011xxxxxb
        Choice "64h" pos[0]=100xxxxxb
        Choice "65h" pos[0]=101xxxxxb
 
       Help
"Use the F5=Previous and F6=Next keys to
 change the Soft Interrupt Vector used by
 the software driving the PSDO board.
 Select a vector number which is currently
 not in use."
 
 
NamedItem
 
       Prompt "16K ROM Assignment for PSDO card"
 
       Choice "C0000-C3FFF" pos[1]=1xxx0000b mem 0c0000h-0c3fffh
       Choice "C4000-C7FFF" pos[1]=1xxx0001b mem 0c4000h-0c7fffh
       Choice "C8000-CBFFF" pos[1]=1xxx0010b mem 0c8000h-0cbfffh
       Choice "CC000-CFFFF" pos[1]=1xxx0011b mem 0cc000h-0cffffh
       Choice "D0000-D3FFF" pos[1]=1xxx0100b mem 0d0000h-0d3fffh
       Choice "D4000-D7FFF" pos[1]=1xxx0101b mem 0d4000h-0d7fffh
       Choice "D8000-DBFFF" pos[1]=1xxx0110b mem 0d8000h-0dbfffh
       Choice "DC000-DFFFF" pos[1]=1xxx0111b mem 0dc000h-0dffffh
 
       Help
"Use the F5=Previous and F6=Next keys to
change the address assignments for the
16K block of onboard ROM."
 
 
NamedItem
 
       Prompt "Interrupt Level for PSDO card"
 
       Choice "Level_7" pos[1]=x011xxxxb int 7
       Choice "Level_3" pos[1]=x000xxxxb int 3
       Choice "Level_4" pos[1]=x001xxxxb int 4
       Choice "Level_5" pos[1]=x010xxxxb int 5
       Choice "Level_9" pos[1]=x100xxxxb int 9
       Choice "Level_10" pos[1]=x101xxxxb int 10
       Choice "Level_11" pos[1]=x110xxxxb int 11
       Choice "Level_15" pos[1]=x111xxxxb int 15
 
       Help
"Use the F5=Previous and F6=Next keys to
 change the interrupt level assignments.
 An interrupt level of 3 has the highest
 priority, and increasing levels have
 corresponding decreased priority."
