
AdapterId 80ECh

AdapterName "Matrox MGA Video Adapter (V0.02)"

NumBytes 2


NamedItem Prompt  "Enable/Disable Adapter"

Choice  " Adapter Enabled "    pos[0]=XXXXXXX1b
Choice  " Adapter Disabled "   pos[0]=XXXXXXX0b

Help

"This controls whether the adapter is enabled or not. Use the Enabled
setting for normal use. Use the Disabled setting if you are not using
the adapter and enabling it causes a conflict with another device."


NamedItem Prompt  "Memory Mapping"

Choice  " Map2 C8000 "         pos[1]=XXXXX010b mem 0c8000h-0cbfffh
Choice  " Map3 CC000 "         pos[1]=XXXXX011b mem 0cc000h-0cffffh
Choice  " Map4 D0000 "         pos[1]=XXXXX100b mem 0d0000h-0d3fffh
Choice  " Map5 D4000 "         pos[1]=XXXXX101b mem 0d4000h-0d7fffh
Choice  " Map6 D8000 "         pos[1]=XXXXX110b mem 0d8000h-0dbfffh
Choice  " Map7 DC000 "         pos[1]=XXXXX111b mem 0dc000h-0dffffh
Choice  " Map1 AC000 "         pos[1]=XXXXX000b 

Help

"There are 7 different 16K windows where you can map the MGA.
Change this setting if it conflicts with another adapter.
Note: Use Map1 only if the on-board VGA is enabled."

NamedItem Prompt  "MGA on-board VGA"

choice  " VGA Enabled "        pos[1]=XXXX0XXXb mem 0c0000h-0c7fffh
choice  " VGA Disabled "       pos[1]=XXXX1XXXb

Help

"Select 'VGA Enabled' if you want a single screen solution.
This setting enables the VGA bios at C0000h (on the MGA adapter)."


NamedItem Prompt  "Composite SYNC"

choice  " CSYNC Disabled "     pos[1]=XXX0XXXXb
choice  " CSYNC Enabled "      pos[1]=XXX1XXXXb

Help

"Select 'CSYNC Enabled' if you are using a composite sync monitor."


NamedItem Prompt  "Zbuffer"

choice  " Zbuffer Absent "     pos[1]=XX0XXXXXb
choice  " Zbuffer Present "    pos[1]=XX1XXXXXb

Help

"Select 'Zbuffer Present' if your MGA has it's ZIP memory installed
on the sockets placed on the lower left area of the adapter.
The default setting is 'Zbuffer Absent'."
