; Madge MCA Ring Node
; Adapter Description File
;
; Version:  1.01
;
; Copyright (c) 1987 Madge Networks Ltd.

AdapterId 0803h
 
AdapterName "Madge MCA Ring Node"
 
NumBytes 2

FixedResources
     POS[1]=10000000b

 
NamedItem Prompt "Primary/Alternate Adapter"
 
  Choice "Alternate - Interrupt Level 9"
     POS[0]=100XXXXXb     IO  1A20h - 1A2Fh     INT  2

  Choice "Alternate - Interrupt Level 3"
     POS[0]=010XXXXXb     IO  1A20h - 1A2Fh     INT  3
 
  Choice "Alternate - Interrupt Level 10"
     POS[0]=110XXXXXb     IO  1A20h - 1A2Fh     INT 10

  Choice "Primary - Interrupt Level 3"
     POS[0]=011XXXXXb     IO  0A20h - 0A2Fh     INT  3

  Choice "Primary - Interrupt Level 10"
     POS[0]=111XXXXXb     IO  0A20h - 0A2Fh     INT 10
 
  Choice "Primary - Interrupt Level 9"
     POS[0]=101XXXXXb     IO  0A20h - 0A2Fh     INT  2
 
  Help "PRIMARY/ALTERNATE ADAPTER: Up to two MCA Ring Nodes may
      be installed. If just one Node is installed, it may be
      set-up as either the Primary or the Alternate adapter;
      if two Nodes are installed, one must be set-up as the
      Primary adapter and the other as the Alternate adapter.

      An MCA Ring Node may share an Interrupt Level with any
      other adapter, but performance may be improved by using
      a different Interrupt Level for each adapter. Use the
      F5=Previous and F6=Next keys to change this assignment
      if you are in the 'Change Configuration' window."


NamedItem Prompt "Arbitration Level"

  Choice "Level 8"   
     POS[0]=XXX1000Xb     ARB  8

  Choice "Level 9"   
     POS[0]=XXX1001Xb     ARB  9

  Choice "Level 10"  
     POS[0]=XXX1010Xb     ARB 10

  Choice "Level 11"  
     POS[0]=XXX1011Xb     ARB 11

  Choice "Level 12"  
     POS[0]=XXX1100Xb     ARB 12

  Choice "Level 13"  
     POS[0]=XXX1101Xb     ARB 13

  Choice "Level 14"  
     POS[0]=XXX1110Xb     ARB 14

  Help "ARBITRATION LEVEL:  The Arbitration Level need only
      be changed if it is in conflict with another adapter.
      Any such conflict is marked with an asterisk. Use the
      F5=Previous and F6=Next keys to change this assignment
      if you are in the 'Change Configuration' window."
